(kicad_pcb (version 20211014) (generator pcbnew)

  (general
    (thickness 1.6)
  )

  (paper "A4")
  (layers
    (0 "F.Cu" signal)
    (31 "B.Cu" signal)
    (32 "B.Adhes" user "B.Adhesive")
    (33 "F.Adhes" user "F.Adhesive")
    (34 "B.Paste" user)
    (35 "F.Paste" user)
    (36 "B.SilkS" user "B.Silkscreen")
    (37 "F.SilkS" user "F.Silkscreen")
    (38 "B.Mask" user)
    (39 "F.Mask" user)
    (40 "Dwgs.User" user "User.Drawings")
    (41 "Cmts.User" user "User.Comments")
    (42 "Eco1.User" user "User.Eco1")
    (43 "Eco2.User" user "User.Eco2")
    (44 "Edge.Cuts" user)
    (45 "Margin" user)
    (46 "B.CrtYd" user "B.Courtyard")
    (47 "F.CrtYd" user "F.Courtyard")
    (48 "B.Fab" user)
    (49 "F.Fab" user)
    (50 "User.1" user)
    (51 "User.2" user)
    (52 "User.3" user)
    (53 "User.4" user)
    (54 "User.5" user)
    (55 "User.6" user)
    (56 "User.7" user)
    (57 "User.8" user)
    (58 "User.9" user)
  )

  (setup
    (stackup
      (layer "F.SilkS" (type "Top Silk Screen"))
      (layer "F.Paste" (type "Top Solder Paste"))
      (layer "F.Mask" (type "Top Solder Mask") (thickness 0.01))
      (layer "F.Cu" (type "copper") (thickness 0.035))
      (layer "dielectric 1" (type "core") (thickness 1.51) (material "FR4") (epsilon_r 4.5) (loss_tangent 0.02))
      (layer "B.Cu" (type "copper") (thickness 0.035))
      (layer "B.Mask" (type "Bottom Solder Mask") (thickness 0.01))
      (layer "B.Paste" (type "Bottom Solder Paste"))
      (layer "B.SilkS" (type "Bottom Silk Screen"))
      (copper_finish "None")
      (dielectric_constraints no)
    )
    (pad_to_mask_clearance 0)
    (pcbplotparams
      (layerselection 0x00010fc_ffffffff)
      (disableapertmacros false)
      (usegerberextensions false)
      (usegerberattributes true)
      (usegerberadvancedattributes true)
      (creategerberjobfile true)
      (svguseinch false)
      (svgprecision 6)
      (excludeedgelayer true)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15.000000)
      (dxfpolygonmode true)
      (dxfimperialunits true)
      (dxfusepcbnewfont true)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (sketchpadsonfab false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 1)
      (scaleselection 1)
      (outputdirectory "")
    )
  )

  (net 0 "")

  (footprint "MountingHole:MountingHole_2.7mm_M2.5_DIN965_Pad_TopOnly" (layer "F.Cu")
    (tedit 56D1B4CB) (tstamp 73c98614-1d86-43b8-81f4-fc5969493654)
    (at 56.5 56.5)
    (descr "Mounting Hole 2.7mm, M2.5, DIN965")
    (tags "mounting hole 2.7mm m2.5 din965")
    (attr exclude_from_pos_files exclude_from_bom)
    (fp_text reference "REF**" (at 0 -3.35) (layer "F.SilkS")
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 5843e3d4-4423-4b84-9ee5-80c77a135f0d)
    )
    (fp_text value "MountingHole_2.7mm_M2.5_DIN965_Pad_TopOnly" (at 0 3.35) (layer "F.Fab")
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 89dcdce5-63b9-476c-a000-897392b6f53c)
    )
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab")
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 86b13b41-51c6-4382-8921-0a4fcf98dab6)
    )
    (fp_circle (center 0 0) (end 2.35 0) (layer "Cmts.User") (width 0.15) (fill none) (tstamp b2a4f826-0e11-45cd-9ea8-e99dd54d0680))
    (fp_circle (center 0 0) (end 2.6 0) (layer "F.CrtYd") (width 0.05) (fill none) (tstamp 8bbe3be6-929f-458e-be18-3d9c80411da1))
    (pad "1" thru_hole circle (at 0 0) (size 3.1 3.1) (drill 2.7) (layers *.Cu *.Mask) (tstamp 9f7ba675-2144-493f-ad3d-fd65a168e759))
    (pad "1" connect circle (at 0 0) (size 4.7 4.7) (layers "F.Cu" "F.Mask") (tstamp d42f2069-605c-4681-9af8-b13179f80008))
  )

  (footprint "MountingHole:MountingHole_2.7mm_M2.5_DIN965_Pad_TopOnly" (layer "F.Cu")
    (tedit 56D1B4CB) (tstamp 87797894-be04-4987-9e54-98f45d945ed1)
    (at 3.5 3.5)
    (descr "Mounting Hole 2.7mm, M2.5, DIN965")
    (tags "mounting hole 2.7mm m2.5 din965")
    (attr exclude_from_pos_files exclude_from_bom)
    (fp_text reference "REF**" (at 0 -3.35) (layer "F.SilkS")
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 23ed9b83-0f31-4b92-8d6e-1b0bc1fcf9ee)
    )
    (fp_text value "MountingHole_2.7mm_M2.5_DIN965_Pad_TopOnly" (at 0 3.35) (layer "F.Fab")
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 4e3b8378-2d3a-4adc-9298-ba4dcf69eb37)
    )
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab")
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 11f69e8f-c7dd-41a3-ba82-394ce8394afd)
    )
    (fp_circle (center 0 0) (end 2.35 0) (layer "Cmts.User") (width 0.15) (fill none) (tstamp e4b1e17c-5f9f-4749-b54e-140ccd253daf))
    (fp_circle (center 0 0) (end 2.6 0) (layer "F.CrtYd") (width 0.05) (fill none) (tstamp 597d72a6-2a02-45c0-b12d-239dbf159efb))
    (pad "1" connect circle (at 0 0) (size 4.7 4.7) (layers "F.Cu" "F.Mask") (tstamp 95171fc6-3095-45f9-b1da-ef1cb350a95d))
    (pad "1" thru_hole circle (at 0 0) (size 3.1 3.1) (drill 2.7) (layers *.Cu *.Mask) (tstamp d6c54596-765b-431c-a40f-aac7d35a7e5e))
  )

  (footprint "MountingHole:MountingHole_2.7mm_M2.5_DIN965_Pad_TopOnly" (layer "F.Cu")
    (tedit 56D1B4CB) (tstamp 9cb81e72-2ca7-4837-a15a-891e6c4c925e)
    (at 3.5 56.5)
    (descr "Mounting Hole 2.7mm, M2.5, DIN965")
    (tags "mounting hole 2.7mm m2.5 din965")
    (attr exclude_from_pos_files exclude_from_bom)
    (fp_text reference "REF**" (at 0 -3.35) (layer "F.SilkS")
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp b5a40e46-9876-4e48-a954-7a4221f0b34e)
    )
    (fp_text value "MountingHole_2.7mm_M2.5_DIN965_Pad_TopOnly" (at 0 3.35) (layer "F.Fab")
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 5c3ed9bd-0024-40d6-9f56-a571058d8f27)
    )
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab")
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp fccf22e6-52d4-47c6-b803-3fd272b15caf)
    )
    (fp_circle (center 0 0) (end 2.35 0) (layer "Cmts.User") (width 0.15) (fill none) (tstamp c06a10fa-aab8-4893-b49e-10951f394902))
    (fp_circle (center 0 0) (end 2.6 0) (layer "F.CrtYd") (width 0.05) (fill none) (tstamp fd626d1b-7066-4bf3-bc56-83eb831ee09c))
    (pad "1" thru_hole circle (at 0 0) (size 3.1 3.1) (drill 2.7) (layers *.Cu *.Mask) (tstamp 5f990dda-61ae-4f7c-96f9-17f36c397386))
    (pad "1" connect circle (at 0 0) (size 4.7 4.7) (layers "F.Cu" "F.Mask") (tstamp 9c493703-1123-4334-9328-52842209b4cf))
  )

  (footprint "MountingHole:MountingHole_2.7mm_M2.5_DIN965_Pad_TopOnly" (layer "F.Cu")
    (tedit 56D1B4CB) (tstamp b83474c6-4446-45d8-b915-14963eb49218)
    (at 56.5 3.5)
    (descr "Mounting Hole 2.7mm, M2.5, DIN965")
    (tags "mounting hole 2.7mm m2.5 din965")
    (attr exclude_from_pos_files exclude_from_bom)
    (fp_text reference "REF**" (at 0 -3.35) (layer "F.SilkS")
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 2fd94add-0249-46fe-8670-53c50e379501)
    )
    (fp_text value "MountingHole_2.7mm_M2.5_DIN965_Pad_TopOnly" (at 0 3.35) (layer "F.Fab")
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp ebc362e9-ed30-4f97-8e97-537451c4c05d)
    )
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab")
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp ef1324cc-4979-46c1-9c01-2c019e5b453e)
    )
    (fp_circle (center 0 0) (end 2.35 0) (layer "Cmts.User") (width 0.15) (fill none) (tstamp fd6e22ce-e5a7-4220-af24-62c3de636608))
    (fp_circle (center 0 0) (end 2.6 0) (layer "F.CrtYd") (width 0.05) (fill none) (tstamp 39ed7e69-9f3e-4d19-9adc-0a07210f3029))
    (pad "1" thru_hole circle (at 0 0) (size 3.1 3.1) (drill 2.7) (layers *.Cu *.Mask) (tstamp 1461d729-5018-4627-8add-6ee17b9c990d))
    (pad "1" connect circle (at 0 0) (size 4.7 4.7) (layers "F.Cu" "F.Mask") (tstamp cebc1c26-ebeb-4ceb-8568-2306ba86b7db))
  )

  (gr_arc (start 57.5 0) (mid 59.267767 0.732233) (end 60 2.5) (layer "Edge.Cuts") (width 0.1) (tstamp 3026f0e5-2e03-4b09-8bf9-bf5e41de9fde))
  (gr_line (start 2.5 60) (end 57.5 60) (layer "Edge.Cuts") (width 0.1) (tstamp 3bc3a1f7-6e8d-4cb1-b522-61dab886a957))
  (gr_line (start 60 57.5) (end 60 2.5) (layer "Edge.Cuts") (width 0.1) (tstamp 55509fb5-1a05-4183-aa48-bc8ee8bff31d))
  (gr_line (start 57.5 0) (end 2.5 0) (layer "Edge.Cuts") (width 0.1) (tstamp a890f558-8662-408a-b127-32740c9a3a78))
  (gr_arc (start 2.5 60) (mid 0.732233 59.267767) (end 0 57.5) (layer "Edge.Cuts") (width 0.1) (tstamp af00085d-1794-4c99-952f-c446aee665f4))
  (gr_arc (start 60 57.5) (mid 59.267767 59.267767) (end 57.5 60) (layer "Edge.Cuts") (width 0.1) (tstamp d4fffbb7-788f-4b07-aa57-4a4d4fff19d5))
  (gr_arc (start 0 2.5) (mid 0.732233 0.732233) (end 2.5 0) (layer "Edge.Cuts") (width 0.1) (tstamp f721f40e-7993-44a7-bcd0-f5608efe0556))

)
