(kicad_pcb (version 20171130) (host pcbnew 5.1.5)

  (general
    (thickness 1.6)
    (drawings 5)
    (tracks 0)
    (zones 0)
    (modules 13)
    (nets 196)
  )

  (page A4)
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal)
    (32 B.Adhes user)
    (33 F.Adhes user)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user)
    (41 Cmts.User user)
    (42 Eco1.User user)
    (43 Eco2.User user)
    (44 Edge.Cuts user)
    (45 Margin user)
    (46 B.CrtYd user)
    (47 F.CrtYd user)
    (48 B.Fab user)
    (49 F.Fab user)
  )

  (setup
    (last_trace_width 0.25)
    (trace_clearance 0.2)
    (zone_clearance 0.508)
    (zone_45_only no)
    (trace_min 0.2)
    (via_size 0.8)
    (via_drill 0.4)
    (via_min_size 0.4)
    (via_min_drill 0.3)
    (uvia_size 0.3)
    (uvia_drill 0.1)
    (uvias_allowed no)
    (uvia_min_size 0.2)
    (uvia_min_drill 0.1)
    (edge_width 0.05)
    (segment_width 0.2)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.12)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 3.45 3.45)
    (pad_drill 0)
    (pad_to_mask_clearance 0.051)
    (solder_mask_min_width 0.25)
    (aux_axis_origin 0 0)
    (visible_elements 7FFFFFFF)
    (pcbplotparams
      (layerselection 0x010fc_ffffffff)
      (usegerberextensions false)
      (usegerberattributes false)
      (usegerberadvancedattributes false)
      (creategerberjobfile false)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15.000000)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 1)
      (scaleselection 1)
      (outputdirectory ""))
  )

  (net 0 "")
  (net 1 "Net-(J1-Pad4)")
  (net 2 "Net-(J2-Pad8)")
  (net 3 "Net-(J2-Pad7)")
  (net 4 "Net-(J2-Pad1)")
  (net 5 "Net-(J3-Pad40)")
  (net 6 "Net-(J3-Pad39)")
  (net 7 "Net-(J3-Pad38)")
  (net 8 "Net-(J3-Pad6)")
  (net 9 "Net-(U1-Pad95)")
  (net 10 "Net-(U1-Pad94)")
  (net 11 "Net-(U1-Pad93)")
  (net 12 "Net-(U1-Pad92)")
  (net 13 "Net-(U1-Pad89)")
  (net 14 "Net-(U1-Pad88)")
  (net 15 "Net-(U1-Pad87)")
  (net 16 "Net-(U1-Pad86)")
  (net 17 "Net-(U1-Pad85)")
  (net 18 "Net-(U1-Pad84)")
  (net 19 "Net-(U1-Pad83)")
  (net 20 "Net-(U1-Pad82)")
  (net 21 "Net-(U1-Pad81)")
  (net 22 "Net-(U1-Pad80)")
  (net 23 "Net-(U1-Pad77)")
  (net 24 "Net-(U1-Pad76)")
  (net 25 "Net-(U1-Pad75)")
  (net 26 "Net-(U1-Pad74)")
  (net 27 "Net-(U1-Pad73)")
  (net 28 "Net-(U1-Pad72)")
  (net 29 "Net-(U1-Pad71)")
  (net 30 "Net-(U1-Pad70)")
  (net 31 "Net-(U1-Pad69)")
  (net 32 "Net-(U1-Pad68)")
  (net 33 "Net-(U1-Pad32)")
  (net 34 "Net-(U1-Pad30)")
  (net 35 "Net-(U1-Pad29)")
  (net 36 "Net-(U1-Pad28)")
  (net 37 "Net-(U1-Pad27)")
  (net 38 "Net-(U1-Pad26)")
  (net 39 "Net-(U1-Pad24)")
  (net 40 "Net-(U1-Pad20)")
  (net 41 "Net-(U1-Pad19)")
  (net 42 "Net-(U1-Pad18)")
  (net 43 "Net-(U1-Pad16)")
  (net 44 "Net-(U1-Pad15)")
  (net 45 "Net-(U1-Pad14)")
  (net 46 "Net-(U1-Pad13)")
  (net 47 "Net-(U1-Pad10)")
  (net 48 "Net-(U1-Pad9)")
  (net 49 "Net-(U1-Pad8)")
  (net 50 "Net-(U1-Pad7)")
  (net 51 "Net-(U1-Pad6)")
  (net 52 "Net-(U1-Pad5)")
  (net 53 "Net-(U1-Pad4)")
  (net 54 "Net-(U1-Pad3)")
  (net 55 "Net-(C1-Pad2)")
  (net 56 "Net-(U1-Pad124)")
  (net 57 "Net-(U1-Pad123)")
  (net 58 "Net-(U1-Pad122)")
  (net 59 "Net-(U1-Pad121)")
  (net 60 "Net-(U1-Pad120)")
  (net 61 "Net-(U1-Pad119)")
  (net 62 "Net-(U1-Pad117)")
  (net 63 "Net-(U1-Pad116)")
  (net 64 "Net-(U1-Pad115)")
  (net 65 "Net-(U1-Pad114)")
  (net 66 "Net-(U1-Pad113)")
  (net 67 "Net-(U1-Pad112)")
  (net 68 "Net-(U1-Pad111)")
  (net 69 "Net-(U1-Pad110)")
  (net 70 "Net-(U1-Pad109)")
  (net 71 "Net-(U1-Pad108)")
  (net 72 "Net-(U1-Pad107)")
  (net 73 "Net-(U1-Pad105)")
  (net 74 "Net-(U1-Pad104)")
  (net 75 "Net-(U1-Pad103)")
  (net 76 "Net-(U1-Pad102)")
  (net 77 "Net-(U1-Pad99)")
  (net 78 "Net-(U1-Pad98)")
  (net 79 "Net-(U1-Pad61)")
  (net 80 "Net-(U1-Pad60)")
  (net 81 "Net-(U1-Pad59)")
  (net 82 "Net-(U1-Pad58)")
  (net 83 "Net-(U1-Pad57)")
  (net 84 "Net-(U1-Pad56)")
  (net 85 "Net-(U1-Pad55)")
  (net 86 "Net-(U1-Pad52)")
  (net 87 "Net-(U1-Pad51)")
  (net 88 "Net-(U1-Pad50)")
  (net 89 "Net-(U1-Pad49)")
  (net 90 "Net-(U1-Pad48)")
  (net 91 "Net-(U1-Pad47)")
  (net 92 "Net-(U1-Pad44)")
  (net 93 "Net-(U1-Pad43)")
  (net 94 "Net-(U1-Pad42)")
  (net 95 "Net-(U1-Pad41)")
  (net 96 "Net-(U1-Pad40)")
  (net 97 "Net-(U1-Pad39)")
  (net 98 "Net-(U1-Pad37)")
  (net 99 "Net-(U1-Pad36)")
  (net 100 "Net-(U1-Pad35)")
  (net 101 "Net-(U1-Pad34)")
  (net 102 "Net-(U1-Pad33)")
  (net 103 "Net-(U2-Pad32)")
  (net 104 "Net-(U2-Pad31)")
  (net 105 "Net-(U2-Pad29)")
  (net 106 "Net-(U2-Pad28)")
  (net 107 "Net-(U2-Pad27)")
  (net 108 "Net-(U2-Pad23)")
  (net 109 "Net-(U2-Pad22)")
  (net 110 "Net-(U2-Pad21)")
  (net 111 "Net-(U2-Pad18)")
  (net 112 "Net-(U2-Pad13)")
  (net 113 "Net-(U2-Pad12)")
  (net 114 "Net-(U2-Pad11)")
  (net 115 "Net-(U2-Pad10)")
  (net 116 "Net-(U2-Pad8)")
  (net 117 "Net-(U2-Pad7)")
  (net 118 "Net-(U2-Pad6)")
  (net 119 "Net-(U2-Pad5)")
  (net 120 "Net-(U2-Pad3)")
  (net 121 "Net-(U2-Pad25)")
  (net 122 g_3v3)
  (net 123 "Net-(U3-Pad32)")
  (net 124 "Net-(U3-Pad31)")
  (net 125 "Net-(U3-Pad30)")
  (net 126 "Net-(U3-Pad29)")
  (net 127 GND)
  (net 128 "Net-(R1-Pad1)")
  (net 129 /s_USB_INTF.sch/USB_D+)
  (net 130 /s_USB_INTF.sch/USB_D-)
  (net 131 "Net-(C2-Pad1)")
  (net 132 "Net-(C5-Pad2)")
  (net 133 "Net-(C4-Pad2)")
  (net 134 /DEBUG_RX)
  (net 135 /DEBUG_TX)
  (net 136 /s_SCREEN_INTF/TFT_STB)
  (net 137 /s_SCREEN_INTF/D23)
  (net 138 /s_SCREEN_INTF/D22)
  (net 139 /s_SCREEN_INTF/D21)
  (net 140 /s_SCREEN_INTF/D20)
  (net 141 /s_SCREEN_INTF/D19)
  (net 142 /s_SCREEN_INTF/D18)
  (net 143 /s_SCREEN_INTF/D17)
  (net 144 /s_SCREEN_INTF/D16)
  (net 145 /s_SCREEN_INTF/D15)
  (net 146 /s_SCREEN_INTF/D14)
  (net 147 /s_SCREEN_INTF/D13)
  (net 148 /s_SCREEN_INTF/D12)
  (net 149 /s_SCREEN_INTF/D11)
  (net 150 /s_SCREEN_INTF/D10)
  (net 151 /s_SCREEN_INTF/D9)
  (net 152 /s_SCREEN_INTF/D8)
  (net 153 /s_SCREEN_INTF/D7)
  (net 154 /s_SCREEN_INTF/D6)
  (net 155 /s_SCREEN_INTF/D5)
  (net 156 /s_SCREEN_INTF/D4)
  (net 157 /s_SCREEN_INTF/D3)
  (net 158 /s_SCREEN_INTF/D2)
  (net 159 /s_SCREEN_INTF/D1)
  (net 160 /s_SCREEN_INTF/D0)
  (net 161 /s_SCREEN_INTF/TFT_TE)
  (net 162 /s_SCREEN_INTF/~TFT_RD)
  (net 163 /s_SCREEN_INTF/~TFT_WR)
  (net 164 /s_SCREEN_INTF/TFT_RSDC)
  (net 165 /s_SCREEN_INTF/~TFT_RST)
  (net 166 /s_SCREEN_INTF/TFT_TOUCH_INT)
  (net 167 /s_SCREEN_INTF/~IO_EXPANDER_CS)
  (net 168 "Net-(C7-Pad1)")
  (net 169 /~TFT_CS)
  (net 170 /MASTER_I2C_SDA)
  (net 171 /MASTER_I2C_SCL)
  (net 172 /s_Power/USB_5v)
  (net 173 /s_Power/USB_3v3)
  (net 174 /MASTER_SPI_MISO)
  (net 175 /MASTER_SPI_CLK)
  (net 176 /s_USB_INTF.sch/FTDI_5V)
  (net 177 /s_USB_INTF.sch/FTDI_3V3)
  (net 178 /MASTER_SPI_MOSI)
  (net 179 "Net-(U4-Pad5)")
  (net 180 "Net-(U4-Pad3)")
  (net 181 "Net-(Q1-Pad3)")
  (net 182 "Net-(Q2-Pad3)")
  (net 183 "Net-(C10-Pad1)")
  (net 184 /s_BRAIN/~SYS_RST)
  (net 185 /s_BRAIN/SWO)
  (net 186 /s_BRAIN/SWCLK)
  (net 187 /s_BRAIN/SWDIO)
  (net 188 /s_Power/Wall_5V)
  (net 189 "Net-(J4-Pad3)")
  (net 190 /s_BRAIN/EXT_IRQ_5)
  (net 191 /s_BRAIN/EXT_IRQ_4)
  (net 192 /s_BRAIN/EXT_IRQ_3)
  (net 193 /s_BRAIN/EXT_IRQ_2)
  (net 194 /s_BRAIN/EXT_IRQ_1)
  (net 195 /s_BRAIN/EXT_IRQ_0)

  (net_class Default "This is the default net class."
    (clearance 0.2)
    (trace_width 0.25)
    (via_dia 0.8)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net /DEBUG_RX)
    (add_net /DEBUG_TX)
    (add_net /MASTER_I2C_SCL)
    (add_net /MASTER_I2C_SDA)
    (add_net /MASTER_SPI_CLK)
    (add_net /MASTER_SPI_MISO)
    (add_net /MASTER_SPI_MOSI)
    (add_net /s_BRAIN/EXT_IRQ_0)
    (add_net /s_BRAIN/EXT_IRQ_1)
    (add_net /s_BRAIN/EXT_IRQ_2)
    (add_net /s_BRAIN/EXT_IRQ_3)
    (add_net /s_BRAIN/EXT_IRQ_4)
    (add_net /s_BRAIN/EXT_IRQ_5)
    (add_net /s_BRAIN/SWCLK)
    (add_net /s_BRAIN/SWDIO)
    (add_net /s_BRAIN/SWO)
    (add_net /s_BRAIN/~SYS_RST)
    (add_net /s_Power/USB_3v3)
    (add_net /s_Power/USB_5v)
    (add_net /s_Power/Wall_5V)
    (add_net /s_SCREEN_INTF/D0)
    (add_net /s_SCREEN_INTF/D1)
    (add_net /s_SCREEN_INTF/D10)
    (add_net /s_SCREEN_INTF/D11)
    (add_net /s_SCREEN_INTF/D12)
    (add_net /s_SCREEN_INTF/D13)
    (add_net /s_SCREEN_INTF/D14)
    (add_net /s_SCREEN_INTF/D15)
    (add_net /s_SCREEN_INTF/D16)
    (add_net /s_SCREEN_INTF/D17)
    (add_net /s_SCREEN_INTF/D18)
    (add_net /s_SCREEN_INTF/D19)
    (add_net /s_SCREEN_INTF/D2)
    (add_net /s_SCREEN_INTF/D20)
    (add_net /s_SCREEN_INTF/D21)
    (add_net /s_SCREEN_INTF/D22)
    (add_net /s_SCREEN_INTF/D23)
    (add_net /s_SCREEN_INTF/D3)
    (add_net /s_SCREEN_INTF/D4)
    (add_net /s_SCREEN_INTF/D5)
    (add_net /s_SCREEN_INTF/D6)
    (add_net /s_SCREEN_INTF/D7)
    (add_net /s_SCREEN_INTF/D8)
    (add_net /s_SCREEN_INTF/D9)
    (add_net /s_SCREEN_INTF/TFT_RSDC)
    (add_net /s_SCREEN_INTF/TFT_STB)
    (add_net /s_SCREEN_INTF/TFT_TE)
    (add_net /s_SCREEN_INTF/TFT_TOUCH_INT)
    (add_net /s_SCREEN_INTF/~IO_EXPANDER_CS)
    (add_net /s_SCREEN_INTF/~TFT_RD)
    (add_net /s_SCREEN_INTF/~TFT_RST)
    (add_net /s_SCREEN_INTF/~TFT_WR)
    (add_net /s_USB_INTF.sch/FTDI_3V3)
    (add_net /s_USB_INTF.sch/FTDI_5V)
    (add_net /s_USB_INTF.sch/USB_D+)
    (add_net /s_USB_INTF.sch/USB_D-)
    (add_net /~TFT_CS)
    (add_net GND)
    (add_net "Net-(C1-Pad2)")
    (add_net "Net-(C10-Pad1)")
    (add_net "Net-(C2-Pad1)")
    (add_net "Net-(C4-Pad2)")
    (add_net "Net-(C5-Pad2)")
    (add_net "Net-(C7-Pad1)")
    (add_net "Net-(J1-Pad4)")
    (add_net "Net-(J2-Pad1)")
    (add_net "Net-(J2-Pad7)")
    (add_net "Net-(J2-Pad8)")
    (add_net "Net-(J3-Pad38)")
    (add_net "Net-(J3-Pad39)")
    (add_net "Net-(J3-Pad40)")
    (add_net "Net-(J3-Pad6)")
    (add_net "Net-(J4-Pad3)")
    (add_net "Net-(Q1-Pad3)")
    (add_net "Net-(Q2-Pad3)")
    (add_net "Net-(R1-Pad1)")
    (add_net "Net-(U1-Pad10)")
    (add_net "Net-(U1-Pad102)")
    (add_net "Net-(U1-Pad103)")
    (add_net "Net-(U1-Pad104)")
    (add_net "Net-(U1-Pad105)")
    (add_net "Net-(U1-Pad107)")
    (add_net "Net-(U1-Pad108)")
    (add_net "Net-(U1-Pad109)")
    (add_net "Net-(U1-Pad110)")
    (add_net "Net-(U1-Pad111)")
    (add_net "Net-(U1-Pad112)")
    (add_net "Net-(U1-Pad113)")
    (add_net "Net-(U1-Pad114)")
    (add_net "Net-(U1-Pad115)")
    (add_net "Net-(U1-Pad116)")
    (add_net "Net-(U1-Pad117)")
    (add_net "Net-(U1-Pad119)")
    (add_net "Net-(U1-Pad120)")
    (add_net "Net-(U1-Pad121)")
    (add_net "Net-(U1-Pad122)")
    (add_net "Net-(U1-Pad123)")
    (add_net "Net-(U1-Pad124)")
    (add_net "Net-(U1-Pad13)")
    (add_net "Net-(U1-Pad14)")
    (add_net "Net-(U1-Pad15)")
    (add_net "Net-(U1-Pad16)")
    (add_net "Net-(U1-Pad18)")
    (add_net "Net-(U1-Pad19)")
    (add_net "Net-(U1-Pad20)")
    (add_net "Net-(U1-Pad24)")
    (add_net "Net-(U1-Pad26)")
    (add_net "Net-(U1-Pad27)")
    (add_net "Net-(U1-Pad28)")
    (add_net "Net-(U1-Pad29)")
    (add_net "Net-(U1-Pad3)")
    (add_net "Net-(U1-Pad30)")
    (add_net "Net-(U1-Pad32)")
    (add_net "Net-(U1-Pad33)")
    (add_net "Net-(U1-Pad34)")
    (add_net "Net-(U1-Pad35)")
    (add_net "Net-(U1-Pad36)")
    (add_net "Net-(U1-Pad37)")
    (add_net "Net-(U1-Pad39)")
    (add_net "Net-(U1-Pad4)")
    (add_net "Net-(U1-Pad40)")
    (add_net "Net-(U1-Pad41)")
    (add_net "Net-(U1-Pad42)")
    (add_net "Net-(U1-Pad43)")
    (add_net "Net-(U1-Pad44)")
    (add_net "Net-(U1-Pad47)")
    (add_net "Net-(U1-Pad48)")
    (add_net "Net-(U1-Pad49)")
    (add_net "Net-(U1-Pad5)")
    (add_net "Net-(U1-Pad50)")
    (add_net "Net-(U1-Pad51)")
    (add_net "Net-(U1-Pad52)")
    (add_net "Net-(U1-Pad55)")
    (add_net "Net-(U1-Pad56)")
    (add_net "Net-(U1-Pad57)")
    (add_net "Net-(U1-Pad58)")
    (add_net "Net-(U1-Pad59)")
    (add_net "Net-(U1-Pad6)")
    (add_net "Net-(U1-Pad60)")
    (add_net "Net-(U1-Pad61)")
    (add_net "Net-(U1-Pad68)")
    (add_net "Net-(U1-Pad69)")
    (add_net "Net-(U1-Pad7)")
    (add_net "Net-(U1-Pad70)")
    (add_net "Net-(U1-Pad71)")
    (add_net "Net-(U1-Pad72)")
    (add_net "Net-(U1-Pad73)")
    (add_net "Net-(U1-Pad74)")
    (add_net "Net-(U1-Pad75)")
    (add_net "Net-(U1-Pad76)")
    (add_net "Net-(U1-Pad77)")
    (add_net "Net-(U1-Pad8)")
    (add_net "Net-(U1-Pad80)")
    (add_net "Net-(U1-Pad81)")
    (add_net "Net-(U1-Pad82)")
    (add_net "Net-(U1-Pad83)")
    (add_net "Net-(U1-Pad84)")
    (add_net "Net-(U1-Pad85)")
    (add_net "Net-(U1-Pad86)")
    (add_net "Net-(U1-Pad87)")
    (add_net "Net-(U1-Pad88)")
    (add_net "Net-(U1-Pad89)")
    (add_net "Net-(U1-Pad9)")
    (add_net "Net-(U1-Pad92)")
    (add_net "Net-(U1-Pad93)")
    (add_net "Net-(U1-Pad94)")
    (add_net "Net-(U1-Pad95)")
    (add_net "Net-(U1-Pad98)")
    (add_net "Net-(U1-Pad99)")
    (add_net "Net-(U2-Pad10)")
    (add_net "Net-(U2-Pad11)")
    (add_net "Net-(U2-Pad12)")
    (add_net "Net-(U2-Pad13)")
    (add_net "Net-(U2-Pad18)")
    (add_net "Net-(U2-Pad21)")
    (add_net "Net-(U2-Pad22)")
    (add_net "Net-(U2-Pad23)")
    (add_net "Net-(U2-Pad25)")
    (add_net "Net-(U2-Pad27)")
    (add_net "Net-(U2-Pad28)")
    (add_net "Net-(U2-Pad29)")
    (add_net "Net-(U2-Pad3)")
    (add_net "Net-(U2-Pad31)")
    (add_net "Net-(U2-Pad32)")
    (add_net "Net-(U2-Pad5)")
    (add_net "Net-(U2-Pad6)")
    (add_net "Net-(U2-Pad7)")
    (add_net "Net-(U2-Pad8)")
    (add_net "Net-(U3-Pad29)")
    (add_net "Net-(U3-Pad30)")
    (add_net "Net-(U3-Pad31)")
    (add_net "Net-(U3-Pad32)")
    (add_net "Net-(U4-Pad3)")
    (add_net "Net-(U4-Pad5)")
    (add_net g_3v3)
  )

  (module digikey-footprints:Barrel_Jack_5.5mmODx2.1mmID_PJ-102A (layer F.Cu) (tedit 5CAD146F) (tstamp 5E7AD729)
    (at 62.23 60.96 90)
    (path /5E7872D3/5E88DD8C)
    (fp_text reference J4 (at 0 -12.1 90) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value Barrel_Jack_Switch (at 0 5.8 90) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start -4.5 3.7) (end 4.5 3.7) (layer F.Fab) (width 0.1))
    (fp_line (start -4.5 3.7) (end -4.5 -10.7) (layer F.Fab) (width 0.1))
    (fp_line (start 4.5 3.7) (end 4.5 -10.7) (layer F.Fab) (width 0.1))
    (fp_line (start -4.5 -10.7) (end 4.5 -10.7) (layer F.Fab) (width 0.1))
    (fp_line (start 4.6 3.8) (end 4.1 3.8) (layer F.SilkS) (width 0.1))
    (fp_line (start 4.6 3.8) (end 4.6 3.3) (layer F.SilkS) (width 0.1))
    (fp_line (start -4.6 3.8) (end -4.1 3.8) (layer F.SilkS) (width 0.1))
    (fp_line (start -4.6 3.8) (end -4.6 3.3) (layer F.SilkS) (width 0.1))
    (fp_line (start -1.2 -1.8) (end 1.2 -1.8) (layer F.SilkS) (width 0.1))
    (fp_line (start -4.6 -10.8) (end -4.6 -10.3) (layer F.SilkS) (width 0.1))
    (fp_line (start -4.6 -10.8) (end -4.1 -10.8) (layer F.SilkS) (width 0.1))
    (fp_line (start 4.6 -10.8) (end 4.1 -10.8) (layer F.SilkS) (width 0.1))
    (fp_line (start 4.6 -10.8) (end 4.6 -10.3) (layer F.SilkS) (width 0.1))
    (fp_line (start -4.6 -3.5) (end -4.6 -4.5) (layer F.SilkS) (width 0.1))
    (fp_line (start 4.6 -3.5) (end 4.6 -4.5) (layer F.SilkS) (width 0.1))
    (fp_line (start -5.9 -10.95) (end 4.8 -10.95) (layer F.CrtYd) (width 0.05))
    (fp_line (start -5.9 -10.95) (end -5.9 4.25) (layer F.CrtYd) (width 0.05))
    (fp_line (start 4.8 -10.95) (end 4.8 4.25) (layer F.CrtYd) (width 0.05))
    (fp_line (start -5.9 4.25) (end 4.8 4.25) (layer F.CrtYd) (width 0.05))
    (pad 2 thru_hole rect (at 0 -3 90) (size 2.6 2) (drill oval 1.6 1) (layers *.Cu *.Mask)
      (net 127 GND))
    (pad 1 thru_hole rect (at 0 3 90) (size 2.6 2) (drill oval 1.6 1) (layers *.Cu *.Mask)
      (net 188 /s_Power/Wall_5V))
    (pad 3 thru_hole rect (at -4.7 0 90) (size 2 2.6) (drill oval 1 1.6) (layers *.Cu *.Mask)
      (net 189 "Net-(J4-Pad3)"))
  )

  (module digikey-footprints:SOT-23-3 (layer F.Cu) (tedit 5D28A5E3) (tstamp 5E7AA6F9)
    (at 72.9 97.79)
    (path /5E7872D3/5E9DB598)
    (attr smd)
    (fp_text reference Q4 (at 0.025 -3.375) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value "Alt PFET_B" (at 0.025 3.25) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start 0.7 1.52) (end 0.7 -1.52) (layer F.Fab) (width 0.1))
    (fp_line (start -0.7 1.52) (end 0.7 1.52) (layer F.Fab) (width 0.1))
    (fp_text user %R (at -0.125 0.15) (layer F.Fab)
      (effects (font (size 0.25 0.25) (thickness 0.05)))
    )
    (fp_line (start 0.825 -1.65) (end 0.825 -1.35) (layer F.SilkS) (width 0.1))
    (fp_line (start 0.45 -1.65) (end 0.825 -1.65) (layer F.SilkS) (width 0.1))
    (fp_line (start 0.825 1.65) (end 0.375 1.65) (layer F.SilkS) (width 0.1))
    (fp_line (start 0.825 1.35) (end 0.825 1.65) (layer F.SilkS) (width 0.1))
    (fp_line (start 0.825 1.425) (end 0.825 1.3) (layer F.SilkS) (width 0.1))
    (fp_line (start -0.825 1.65) (end -0.825 1.3) (layer F.SilkS) (width 0.1))
    (fp_line (start -0.35 1.65) (end -0.825 1.65) (layer F.SilkS) (width 0.1))
    (fp_line (start -0.425 -1.525) (end -0.7 -1.325) (layer F.Fab) (width 0.1))
    (fp_line (start -0.425 -1.525) (end 0.7 -1.525) (layer F.Fab) (width 0.1))
    (fp_line (start -0.7 -1.325) (end -0.7 1.525) (layer F.Fab) (width 0.1))
    (fp_line (start -0.825 -1.325) (end -1.6 -1.325) (layer F.SilkS) (width 0.1))
    (fp_line (start -0.825 -1.375) (end -0.825 -1.325) (layer F.SilkS) (width 0.1))
    (fp_line (start -0.45 -1.65) (end -0.825 -1.375) (layer F.SilkS) (width 0.1))
    (fp_line (start -0.175 -1.65) (end -0.45 -1.65) (layer F.SilkS) (width 0.1))
    (fp_line (start 1.825 -1.95) (end 1.825 1.95) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.825 1.95) (end -1.825 1.95) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.825 -1.95) (end -1.825 1.95) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.825 -1.95) (end 1.825 -1.95) (layer F.CrtYd) (width 0.05))
    (pad 1 smd rect (at -1.05 -0.95) (size 1.3 0.6) (layers F.Cu F.Paste F.Mask)
      (net 181 "Net-(Q1-Pad3)") (solder_mask_margin 0.07))
    (pad 2 smd rect (at -1.05 0.95) (size 1.3 0.6) (layers F.Cu F.Paste F.Mask)
      (net 183 "Net-(C10-Pad1)") (solder_mask_margin 0.07))
    (pad 3 smd rect (at 1.05 0) (size 1.3 0.6) (layers F.Cu F.Paste F.Mask)
      (net 182 "Net-(Q2-Pad3)") (solder_mask_margin 0.07))
  )

  (module digikey-footprints:SOT-23-3 (layer F.Cu) (tedit 5D28A5E3) (tstamp 5E7AA6DD)
    (at 68.2 97.79)
    (path /5E7872D3/5E9CBFD6)
    (attr smd)
    (fp_text reference Q3 (at 0.025 -3.375) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value "Default PFET_B" (at 0.025 3.25) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start 0.7 1.52) (end 0.7 -1.52) (layer F.Fab) (width 0.1))
    (fp_line (start -0.7 1.52) (end 0.7 1.52) (layer F.Fab) (width 0.1))
    (fp_text user %R (at -0.125 0.15) (layer F.Fab)
      (effects (font (size 0.25 0.25) (thickness 0.05)))
    )
    (fp_line (start 0.825 -1.65) (end 0.825 -1.35) (layer F.SilkS) (width 0.1))
    (fp_line (start 0.45 -1.65) (end 0.825 -1.65) (layer F.SilkS) (width 0.1))
    (fp_line (start 0.825 1.65) (end 0.375 1.65) (layer F.SilkS) (width 0.1))
    (fp_line (start 0.825 1.35) (end 0.825 1.65) (layer F.SilkS) (width 0.1))
    (fp_line (start 0.825 1.425) (end 0.825 1.3) (layer F.SilkS) (width 0.1))
    (fp_line (start -0.825 1.65) (end -0.825 1.3) (layer F.SilkS) (width 0.1))
    (fp_line (start -0.35 1.65) (end -0.825 1.65) (layer F.SilkS) (width 0.1))
    (fp_line (start -0.425 -1.525) (end -0.7 -1.325) (layer F.Fab) (width 0.1))
    (fp_line (start -0.425 -1.525) (end 0.7 -1.525) (layer F.Fab) (width 0.1))
    (fp_line (start -0.7 -1.325) (end -0.7 1.525) (layer F.Fab) (width 0.1))
    (fp_line (start -0.825 -1.325) (end -1.6 -1.325) (layer F.SilkS) (width 0.1))
    (fp_line (start -0.825 -1.375) (end -0.825 -1.325) (layer F.SilkS) (width 0.1))
    (fp_line (start -0.45 -1.65) (end -0.825 -1.375) (layer F.SilkS) (width 0.1))
    (fp_line (start -0.175 -1.65) (end -0.45 -1.65) (layer F.SilkS) (width 0.1))
    (fp_line (start 1.825 -1.95) (end 1.825 1.95) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.825 1.95) (end -1.825 1.95) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.825 -1.95) (end -1.825 1.95) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.825 -1.95) (end 1.825 -1.95) (layer F.CrtYd) (width 0.05))
    (pad 1 smd rect (at -1.05 -0.95) (size 1.3 0.6) (layers F.Cu F.Paste F.Mask)
      (net 173 /s_Power/USB_3v3) (solder_mask_margin 0.07))
    (pad 2 smd rect (at -1.05 0.95) (size 1.3 0.6) (layers F.Cu F.Paste F.Mask)
      (net 183 "Net-(C10-Pad1)") (solder_mask_margin 0.07))
    (pad 3 smd rect (at 1.05 0) (size 1.3 0.6) (layers F.Cu F.Paste F.Mask)
      (net 181 "Net-(Q1-Pad3)") (solder_mask_margin 0.07))
  )

  (module digikey-footprints:SOT-23-3 (layer F.Cu) (tedit 5D28A5E3) (tstamp 5E7AA6C1)
    (at 63.5 102.74)
    (path /5E7872D3/5E9D56A5)
    (attr smd)
    (fp_text reference Q2 (at 0.025 -3.375) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value "Alt PFET_A" (at 0.025 3.25) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start 0.7 1.52) (end 0.7 -1.52) (layer F.Fab) (width 0.1))
    (fp_line (start -0.7 1.52) (end 0.7 1.52) (layer F.Fab) (width 0.1))
    (fp_text user %R (at -0.125 0.15) (layer F.Fab)
      (effects (font (size 0.25 0.25) (thickness 0.05)))
    )
    (fp_line (start 0.825 -1.65) (end 0.825 -1.35) (layer F.SilkS) (width 0.1))
    (fp_line (start 0.45 -1.65) (end 0.825 -1.65) (layer F.SilkS) (width 0.1))
    (fp_line (start 0.825 1.65) (end 0.375 1.65) (layer F.SilkS) (width 0.1))
    (fp_line (start 0.825 1.35) (end 0.825 1.65) (layer F.SilkS) (width 0.1))
    (fp_line (start 0.825 1.425) (end 0.825 1.3) (layer F.SilkS) (width 0.1))
    (fp_line (start -0.825 1.65) (end -0.825 1.3) (layer F.SilkS) (width 0.1))
    (fp_line (start -0.35 1.65) (end -0.825 1.65) (layer F.SilkS) (width 0.1))
    (fp_line (start -0.425 -1.525) (end -0.7 -1.325) (layer F.Fab) (width 0.1))
    (fp_line (start -0.425 -1.525) (end 0.7 -1.525) (layer F.Fab) (width 0.1))
    (fp_line (start -0.7 -1.325) (end -0.7 1.525) (layer F.Fab) (width 0.1))
    (fp_line (start -0.825 -1.325) (end -1.6 -1.325) (layer F.SilkS) (width 0.1))
    (fp_line (start -0.825 -1.375) (end -0.825 -1.325) (layer F.SilkS) (width 0.1))
    (fp_line (start -0.45 -1.65) (end -0.825 -1.375) (layer F.SilkS) (width 0.1))
    (fp_line (start -0.175 -1.65) (end -0.45 -1.65) (layer F.SilkS) (width 0.1))
    (fp_line (start 1.825 -1.95) (end 1.825 1.95) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.825 1.95) (end -1.825 1.95) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.825 -1.95) (end -1.825 1.95) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.825 -1.95) (end 1.825 -1.95) (layer F.CrtYd) (width 0.05))
    (pad 1 smd rect (at -1.05 -0.95) (size 1.3 0.6) (layers F.Cu F.Paste F.Mask)
      (net 181 "Net-(Q1-Pad3)") (solder_mask_margin 0.07))
    (pad 2 smd rect (at -1.05 0.95) (size 1.3 0.6) (layers F.Cu F.Paste F.Mask)
      (net 173 /s_Power/USB_3v3) (solder_mask_margin 0.07))
    (pad 3 smd rect (at 1.05 0) (size 1.3 0.6) (layers F.Cu F.Paste F.Mask)
      (net 182 "Net-(Q2-Pad3)") (solder_mask_margin 0.07))
  )

  (module digikey-footprints:SOT-23-3 (layer F.Cu) (tedit 5D28A5E3) (tstamp 5E7AA6A5)
    (at 69.85 82.55)
    (path /5E7872D3/5E9B8E9E)
    (attr smd)
    (fp_text reference Q1 (at 0.025 -3.375) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value "Default PFET_A" (at 0.025 3.25) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start 0.7 1.52) (end 0.7 -1.52) (layer F.Fab) (width 0.1))
    (fp_line (start -0.7 1.52) (end 0.7 1.52) (layer F.Fab) (width 0.1))
    (fp_text user %R (at -0.125 0.15) (layer F.Fab)
      (effects (font (size 0.25 0.25) (thickness 0.05)))
    )
    (fp_line (start 0.825 -1.65) (end 0.825 -1.35) (layer F.SilkS) (width 0.1))
    (fp_line (start 0.45 -1.65) (end 0.825 -1.65) (layer F.SilkS) (width 0.1))
    (fp_line (start 0.825 1.65) (end 0.375 1.65) (layer F.SilkS) (width 0.1))
    (fp_line (start 0.825 1.35) (end 0.825 1.65) (layer F.SilkS) (width 0.1))
    (fp_line (start 0.825 1.425) (end 0.825 1.3) (layer F.SilkS) (width 0.1))
    (fp_line (start -0.825 1.65) (end -0.825 1.3) (layer F.SilkS) (width 0.1))
    (fp_line (start -0.35 1.65) (end -0.825 1.65) (layer F.SilkS) (width 0.1))
    (fp_line (start -0.425 -1.525) (end -0.7 -1.325) (layer F.Fab) (width 0.1))
    (fp_line (start -0.425 -1.525) (end 0.7 -1.525) (layer F.Fab) (width 0.1))
    (fp_line (start -0.7 -1.325) (end -0.7 1.525) (layer F.Fab) (width 0.1))
    (fp_line (start -0.825 -1.325) (end -1.6 -1.325) (layer F.SilkS) (width 0.1))
    (fp_line (start -0.825 -1.375) (end -0.825 -1.325) (layer F.SilkS) (width 0.1))
    (fp_line (start -0.45 -1.65) (end -0.825 -1.375) (layer F.SilkS) (width 0.1))
    (fp_line (start -0.175 -1.65) (end -0.45 -1.65) (layer F.SilkS) (width 0.1))
    (fp_line (start 1.825 -1.95) (end 1.825 1.95) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.825 1.95) (end -1.825 1.95) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.825 -1.95) (end -1.825 1.95) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.825 -1.95) (end 1.825 -1.95) (layer F.CrtYd) (width 0.05))
    (pad 1 smd rect (at -1.05 -0.95) (size 1.3 0.6) (layers F.Cu F.Paste F.Mask)
      (net 173 /s_Power/USB_3v3) (solder_mask_margin 0.07))
    (pad 2 smd rect (at -1.05 0.95) (size 1.3 0.6) (layers F.Cu F.Paste F.Mask)
      (net 172 /s_Power/USB_5v) (solder_mask_margin 0.07))
    (pad 3 smd rect (at 1.05 0) (size 1.3 0.6) (layers F.Cu F.Paste F.Mask)
      (net 181 "Net-(Q1-Pad3)") (solder_mask_margin 0.07))
  )

  (module Package_DFN_QFN:DFN-6-1EP_2x2mm_P0.65mm_EP1x1.6mm (layer F.Cu) (tedit 5A64E13E) (tstamp 5E7A9FEB)
    (at 80.01 71.12)
    (descr "6-Lead Plastic Dual Flat, No Lead Package (MA) - 2x2x0.9 mm Body [DFN] (see Microchip Packaging Specification 00000049BS.pdf)")
    (tags "DFN 0.65")
    (path /5E7872D3/5E7F2428)
    (attr smd)
    (fp_text reference U4 (at 0 -2.025) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value NCP349MNAETBG (at 0 2.025) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start -1.45 -1.1) (end 0.725 -1.1) (layer F.SilkS) (width 0.15))
    (fp_line (start -0.725 1.1) (end 0.725 1.1) (layer F.SilkS) (width 0.15))
    (fp_line (start -1.65 1.25) (end 1.65 1.25) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.65 -1.25) (end 1.65 -1.25) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.65 -1.25) (end 1.65 1.25) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.65 -1.25) (end -1.65 1.25) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1 0) (end 0 -1) (layer F.Fab) (width 0.15))
    (fp_line (start -1 1) (end -1 0) (layer F.Fab) (width 0.15))
    (fp_line (start 1 1) (end -1 1) (layer F.Fab) (width 0.15))
    (fp_line (start 1 -1) (end 1 1) (layer F.Fab) (width 0.15))
    (fp_line (start 0 -1) (end 1 -1) (layer F.Fab) (width 0.15))
    (fp_text user %R (at 0 0) (layer F.Fab)
      (effects (font (size 0.5 0.5) (thickness 0.075)))
    )
    (pad "" smd rect (at 0 0.4) (size 0.82 0.63) (layers F.Paste))
    (pad "" smd rect (at 0 -0.4) (size 0.82 0.63) (layers F.Paste))
    (pad 7 smd rect (at 0 0) (size 1 1.6) (layers F.Cu F.Mask))
    (pad 6 smd rect (at 1.05 -0.65) (size 0.65 0.35) (layers F.Cu F.Paste F.Mask)
      (net 179 "Net-(U4-Pad5)"))
    (pad 5 smd rect (at 1.05 0) (size 0.65 0.35) (layers F.Cu F.Paste F.Mask)
      (net 179 "Net-(U4-Pad5)"))
    (pad 4 smd rect (at 1.05 0.65) (size 0.65 0.35) (layers F.Cu F.Paste F.Mask)
      (net 127 GND))
    (pad 3 smd rect (at -1.05 0.65) (size 0.65 0.35) (layers F.Cu F.Paste F.Mask)
      (net 180 "Net-(U4-Pad3)"))
    (pad 2 smd rect (at -1.05 0) (size 0.65 0.35) (layers F.Cu F.Paste F.Mask)
      (net 127 GND))
    (pad 1 smd rect (at -1.05 -0.65) (size 0.65 0.35) (layers F.Cu F.Paste F.Mask)
      (net 183 "Net-(C10-Pad1)"))
    (model ${KISYS3DMOD}/Package_DFN_QFN.3dshapes/DFN-6-1EP_2x2mm_P0.65mm_EP1x1.6mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Connector_PinHeader_1.27mm:PinHeader_2x05_P1.27mm_Vertical (layer F.Cu) (tedit 59FED6E3) (tstamp 5E75429F)
    (at 128.27 83.82)
    (descr "Through hole straight pin header, 2x05, 1.27mm pitch, double rows")
    (tags "Through hole pin header THT 2x05 1.27mm double row")
    (path /5E805E4F/5EA1E350)
    (fp_text reference J2 (at 0.635 -1.695) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value Conn_ARM_JTAG_SWD_10 (at 0.635 6.775) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text user %R (at 0.635 2.54 90) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start 2.85 -1.15) (end -1.6 -1.15) (layer F.CrtYd) (width 0.05))
    (fp_line (start 2.85 6.25) (end 2.85 -1.15) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.6 6.25) (end 2.85 6.25) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.6 -1.15) (end -1.6 6.25) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.13 -0.76) (end 0 -0.76) (layer F.SilkS) (width 0.12))
    (fp_line (start -1.13 0) (end -1.13 -0.76) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.57753 -0.695) (end 2.4 -0.695) (layer F.SilkS) (width 0.12))
    (fp_line (start 0.76 -0.695) (end 0.96247 -0.695) (layer F.SilkS) (width 0.12))
    (fp_line (start 0.76 -0.563471) (end 0.76 -0.695) (layer F.SilkS) (width 0.12))
    (fp_line (start 0.76 0.706529) (end 0.76 0.563471) (layer F.SilkS) (width 0.12))
    (fp_line (start 0.563471 0.76) (end 0.706529 0.76) (layer F.SilkS) (width 0.12))
    (fp_line (start -1.13 0.76) (end -0.563471 0.76) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.4 -0.695) (end 2.4 5.775) (layer F.SilkS) (width 0.12))
    (fp_line (start -1.13 0.76) (end -1.13 5.775) (layer F.SilkS) (width 0.12))
    (fp_line (start 0.30753 5.775) (end 0.96247 5.775) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.57753 5.775) (end 2.4 5.775) (layer F.SilkS) (width 0.12))
    (fp_line (start -1.13 5.775) (end -0.30753 5.775) (layer F.SilkS) (width 0.12))
    (fp_line (start -1.07 0.2175) (end -0.2175 -0.635) (layer F.Fab) (width 0.1))
    (fp_line (start -1.07 5.715) (end -1.07 0.2175) (layer F.Fab) (width 0.1))
    (fp_line (start 2.34 5.715) (end -1.07 5.715) (layer F.Fab) (width 0.1))
    (fp_line (start 2.34 -0.635) (end 2.34 5.715) (layer F.Fab) (width 0.1))
    (fp_line (start -0.2175 -0.635) (end 2.34 -0.635) (layer F.Fab) (width 0.1))
    (pad 10 thru_hole oval (at 1.27 5.08) (size 1 1) (drill 0.65) (layers *.Cu *.Mask)
      (net 184 /s_BRAIN/~SYS_RST))
    (pad 9 thru_hole oval (at 0 5.08) (size 1 1) (drill 0.65) (layers *.Cu *.Mask)
      (net 127 GND))
    (pad 8 thru_hole oval (at 1.27 3.81) (size 1 1) (drill 0.65) (layers *.Cu *.Mask)
      (net 2 "Net-(J2-Pad8)"))
    (pad 7 thru_hole oval (at 0 3.81) (size 1 1) (drill 0.65) (layers *.Cu *.Mask)
      (net 3 "Net-(J2-Pad7)"))
    (pad 6 thru_hole oval (at 1.27 2.54) (size 1 1) (drill 0.65) (layers *.Cu *.Mask)
      (net 185 /s_BRAIN/SWO))
    (pad 5 thru_hole oval (at 0 2.54) (size 1 1) (drill 0.65) (layers *.Cu *.Mask)
      (net 127 GND))
    (pad 4 thru_hole oval (at 1.27 1.27) (size 1 1) (drill 0.65) (layers *.Cu *.Mask)
      (net 186 /s_BRAIN/SWCLK))
    (pad 3 thru_hole oval (at 0 1.27) (size 1 1) (drill 0.65) (layers *.Cu *.Mask)
      (net 127 GND))
    (pad 2 thru_hole oval (at 1.27 0) (size 1 1) (drill 0.65) (layers *.Cu *.Mask)
      (net 187 /s_BRAIN/SWDIO))
    (pad 1 thru_hole rect (at 0 0) (size 1 1) (drill 0.65) (layers *.Cu *.Mask)
      (net 4 "Net-(J2-Pad1)"))
    (model ${KISYS3DMOD}/Connector_PinHeader_1.27mm.3dshapes/PinHeader_2x05_P1.27mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Crystal:Crystal_SMD_3215-2Pin_3.2x1.5mm (layer F.Cu) (tedit 5A0FD1B2) (tstamp 5E752FF8)
    (at 63.5 86.36)
    (descr "SMD Crystal FC-135 https://support.epson.biz/td/api/doc_check.php?dl=brief_FC-135R_en.pdf")
    (tags "SMD SMT Crystal")
    (path /5E805E4F/5E75D825)
    (attr smd)
    (fp_text reference Y1 (at 0 -2) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value XOSC32 (at 0 2) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start 2 -1.15) (end 2 1.15) (layer F.CrtYd) (width 0.05))
    (fp_line (start -2 -1.15) (end -2 1.15) (layer F.CrtYd) (width 0.05))
    (fp_line (start -2 1.15) (end 2 1.15) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.6 0.75) (end 1.6 0.75) (layer F.Fab) (width 0.1))
    (fp_line (start -1.6 -0.75) (end 1.6 -0.75) (layer F.Fab) (width 0.1))
    (fp_line (start 1.6 -0.75) (end 1.6 0.75) (layer F.Fab) (width 0.1))
    (fp_line (start -0.675 -0.875) (end 0.675 -0.875) (layer F.SilkS) (width 0.12))
    (fp_line (start -0.675 0.875) (end 0.675 0.875) (layer F.SilkS) (width 0.12))
    (fp_line (start -1.6 -0.75) (end -1.6 0.75) (layer F.Fab) (width 0.1))
    (fp_line (start -2 -1.15) (end 2 -1.15) (layer F.CrtYd) (width 0.05))
    (fp_text user %R (at 0 -2) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (pad 2 smd rect (at -1.25 0) (size 1 1.8) (layers F.Cu F.Paste F.Mask)
      (net 55 "Net-(C1-Pad2)"))
    (pad 1 smd rect (at 1.25 0) (size 1 1.8) (layers F.Cu F.Paste F.Mask)
      (net 131 "Net-(C2-Pad1)"))
    (model ${KISYS3DMOD}/Crystal.3dshapes/Crystal_SMD_3215-2Pin_3.2x1.5mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module proj_modules:SOP80P1030X264-36N (layer F.Cu) (tedit 5E702418) (tstamp 5E752FE7)
    (at 106.68 77.47)
    (path /5E8589A7/5E86D6D7)
    (fp_text reference U3 (at -2.415 -8.587) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.015)))
    )
    (fp_text value MAX7301AAX+ (at 5.84 8.587) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.015)))
    )
    (fp_line (start 5.865 -8.025) (end 5.865 8.025) (layer F.CrtYd) (width 0.05))
    (fp_line (start -5.865 -8.025) (end -5.865 8.025) (layer F.CrtYd) (width 0.05))
    (fp_line (start -5.865 8.025) (end 5.865 8.025) (layer F.CrtYd) (width 0.05))
    (fp_line (start -5.865 -8.025) (end 5.865 -8.025) (layer F.CrtYd) (width 0.05))
    (fp_line (start 3.8 -7.775) (end 3.8 7.775) (layer F.Fab) (width 0.127))
    (fp_line (start -3.8 -7.775) (end -3.8 7.775) (layer F.Fab) (width 0.127))
    (fp_line (start -3.8 7.775) (end 3.8 7.775) (layer F.SilkS) (width 0.127))
    (fp_line (start -3.8 -7.775) (end 3.8 -7.775) (layer F.SilkS) (width 0.127))
    (fp_line (start -3.8 7.775) (end 3.8 7.775) (layer F.Fab) (width 0.127))
    (fp_line (start -3.8 -7.775) (end 3.8 -7.775) (layer F.Fab) (width 0.127))
    (fp_circle (center -6.51 -7.34) (end -6.41 -7.34) (layer F.Fab) (width 0.2))
    (fp_circle (center -6.51 -7.34) (end -6.41 -7.34) (layer F.SilkS) (width 0.2))
    (pad 36 smd rect (at 4.72 -6.8) (size 1.79 0.54) (layers F.Cu F.Paste F.Mask)
      (net 122 g_3v3))
    (pad 35 smd rect (at 4.72 -6) (size 1.79 0.54) (layers F.Cu F.Paste F.Mask)
      (net 167 /s_SCREEN_INTF/~IO_EXPANDER_CS))
    (pad 34 smd rect (at 4.72 -5.2) (size 1.79 0.54) (layers F.Cu F.Paste F.Mask)
      (net 178 /MASTER_SPI_MOSI))
    (pad 33 smd rect (at 4.72 -4.4) (size 1.79 0.54) (layers F.Cu F.Paste F.Mask)
      (net 175 /MASTER_SPI_CLK))
    (pad 32 smd rect (at 4.72 -3.6) (size 1.79 0.54) (layers F.Cu F.Paste F.Mask)
      (net 123 "Net-(U3-Pad32)"))
    (pad 31 smd rect (at 4.72 -2.8) (size 1.79 0.54) (layers F.Cu F.Paste F.Mask)
      (net 124 "Net-(U3-Pad31)"))
    (pad 30 smd rect (at 4.72 -2) (size 1.79 0.54) (layers F.Cu F.Paste F.Mask)
      (net 125 "Net-(U3-Pad30)"))
    (pad 29 smd rect (at 4.72 -1.2) (size 1.79 0.54) (layers F.Cu F.Paste F.Mask)
      (net 126 "Net-(U3-Pad29)"))
    (pad 28 smd rect (at 4.72 -0.4) (size 1.79 0.54) (layers F.Cu F.Paste F.Mask)
      (net 137 /s_SCREEN_INTF/D23))
    (pad 27 smd rect (at 4.72 0.4) (size 1.79 0.54) (layers F.Cu F.Paste F.Mask)
      (net 138 /s_SCREEN_INTF/D22))
    (pad 26 smd rect (at 4.72 1.2) (size 1.79 0.54) (layers F.Cu F.Paste F.Mask)
      (net 139 /s_SCREEN_INTF/D21))
    (pad 25 smd rect (at 4.72 2) (size 1.79 0.54) (layers F.Cu F.Paste F.Mask)
      (net 140 /s_SCREEN_INTF/D20))
    (pad 24 smd rect (at 4.72 2.8) (size 1.79 0.54) (layers F.Cu F.Paste F.Mask)
      (net 141 /s_SCREEN_INTF/D19))
    (pad 23 smd rect (at 4.72 3.6) (size 1.79 0.54) (layers F.Cu F.Paste F.Mask)
      (net 142 /s_SCREEN_INTF/D18))
    (pad 22 smd rect (at 4.72 4.4) (size 1.79 0.54) (layers F.Cu F.Paste F.Mask)
      (net 143 /s_SCREEN_INTF/D17))
    (pad 21 smd rect (at 4.72 5.2) (size 1.79 0.54) (layers F.Cu F.Paste F.Mask)
      (net 144 /s_SCREEN_INTF/D16))
    (pad 20 smd rect (at 4.72 6) (size 1.79 0.54) (layers F.Cu F.Paste F.Mask)
      (net 145 /s_SCREEN_INTF/D15))
    (pad 19 smd rect (at 4.72 6.8) (size 1.79 0.54) (layers F.Cu F.Paste F.Mask)
      (net 146 /s_SCREEN_INTF/D14))
    (pad 18 smd rect (at -4.72 6.8) (size 1.79 0.54) (layers F.Cu F.Paste F.Mask)
      (net 147 /s_SCREEN_INTF/D13))
    (pad 17 smd rect (at -4.72 6) (size 1.79 0.54) (layers F.Cu F.Paste F.Mask)
      (net 148 /s_SCREEN_INTF/D12))
    (pad 16 smd rect (at -4.72 5.2) (size 1.79 0.54) (layers F.Cu F.Paste F.Mask)
      (net 149 /s_SCREEN_INTF/D11))
    (pad 15 smd rect (at -4.72 4.4) (size 1.79 0.54) (layers F.Cu F.Paste F.Mask)
      (net 150 /s_SCREEN_INTF/D10))
    (pad 14 smd rect (at -4.72 3.6) (size 1.79 0.54) (layers F.Cu F.Paste F.Mask)
      (net 151 /s_SCREEN_INTF/D9))
    (pad 13 smd rect (at -4.72 2.8) (size 1.79 0.54) (layers F.Cu F.Paste F.Mask)
      (net 152 /s_SCREEN_INTF/D8))
    (pad 12 smd rect (at -4.72 2) (size 1.79 0.54) (layers F.Cu F.Paste F.Mask)
      (net 153 /s_SCREEN_INTF/D7))
    (pad 11 smd rect (at -4.72 1.2) (size 1.79 0.54) (layers F.Cu F.Paste F.Mask)
      (net 154 /s_SCREEN_INTF/D6))
    (pad 10 smd rect (at -4.72 0.4) (size 1.79 0.54) (layers F.Cu F.Paste F.Mask)
      (net 155 /s_SCREEN_INTF/D5))
    (pad 9 smd rect (at -4.72 -0.4) (size 1.79 0.54) (layers F.Cu F.Paste F.Mask)
      (net 156 /s_SCREEN_INTF/D4))
    (pad 8 smd rect (at -4.72 -1.2) (size 1.79 0.54) (layers F.Cu F.Paste F.Mask)
      (net 157 /s_SCREEN_INTF/D3))
    (pad 7 smd rect (at -4.72 -2) (size 1.79 0.54) (layers F.Cu F.Paste F.Mask)
      (net 158 /s_SCREEN_INTF/D2))
    (pad 6 smd rect (at -4.72 -2.8) (size 1.79 0.54) (layers F.Cu F.Paste F.Mask)
      (net 159 /s_SCREEN_INTF/D1))
    (pad 5 smd rect (at -4.72 -3.6) (size 1.79 0.54) (layers F.Cu F.Paste F.Mask)
      (net 160 /s_SCREEN_INTF/D0))
    (pad 4 smd rect (at -4.72 -4.4) (size 1.79 0.54) (layers F.Cu F.Paste F.Mask)
      (net 174 /MASTER_SPI_MISO))
    (pad 3 smd rect (at -4.72 -5.2) (size 1.79 0.54) (layers F.Cu F.Paste F.Mask)
      (net 127 GND))
    (pad 2 smd rect (at -4.72 -6) (size 1.79 0.54) (layers F.Cu F.Paste F.Mask)
      (net 127 GND))
    (pad 1 smd rect (at -4.72 -6.8) (size 1.79 0.54) (layers F.Cu F.Paste F.Mask)
      (net 128 "Net-(R1-Pad1)"))
  )

  (module digikey-footprints:QFN-32-1EP_5x5mm (layer F.Cu) (tedit 5D2895FE) (tstamp 5E752FB3)
    (at 71.12 73.66)
    (path /5E7C0F59/5E84744C)
    (attr smd)
    (fp_text reference U2 (at 0 -4.71) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value FT232RQ-REEL (at 0 4.51) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start 1.98 2.05) (end -3.02 2.05) (layer F.Fab) (width 0.1))
    (fp_line (start 1.98 -2.95) (end 1.98 2.05) (layer F.Fab) (width 0.1))
    (fp_line (start 2.08 2.15) (end 1.68 2.15) (layer F.SilkS) (width 0.1))
    (fp_line (start 2.08 1.75) (end 2.08 2.15) (layer F.SilkS) (width 0.1))
    (fp_line (start 2.08 -3.05) (end 2.08 -2.65) (layer F.SilkS) (width 0.1))
    (fp_line (start 2.08 -3.05) (end 1.68 -3.05) (layer F.SilkS) (width 0.1))
    (fp_line (start -3.12 2.15) (end -3.12 1.75) (layer F.SilkS) (width 0.1))
    (fp_line (start -2.72 2.15) (end -3.12 2.15) (layer F.SilkS) (width 0.1))
    (fp_line (start -2.62 -2.95) (end -3.02 -2.55) (layer F.Fab) (width 0.1))
    (fp_line (start -3.02 -2.55) (end -3.02 2.05) (layer F.Fab) (width 0.1))
    (fp_line (start -2.62 -2.95) (end 1.98 -2.95) (layer F.Fab) (width 0.1))
    (fp_line (start -3.12 -2.45) (end -3.32 -2.45) (layer F.SilkS) (width 0.1))
    (fp_line (start -3.12 -2.65) (end -3.12 -2.45) (layer F.SilkS) (width 0.1))
    (fp_line (start -2.72 -3.05) (end -3.12 -2.65) (layer F.SilkS) (width 0.1))
    (fp_line (start -2.52 -3.05) (end -2.72 -3.05) (layer F.SilkS) (width 0.1))
    (fp_text user %R (at -0.52 -0.45) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start 2.61 2.68) (end -3.65 2.68) (layer F.CrtYd) (width 0.05))
    (fp_line (start 2.61 -3.58) (end -3.65 -3.58) (layer F.CrtYd) (width 0.05))
    (fp_line (start 2.61 -3.58) (end 2.61 2.68) (layer F.CrtYd) (width 0.05))
    (fp_line (start -3.65 2.68) (end -3.65 -3.58) (layer F.CrtYd) (width 0.05))
    (pad 32 smd rect (at -2.27 -2.925 270) (size 0.85 0.28) (layers F.Cu F.Paste F.Mask)
      (net 103 "Net-(U2-Pad32)") (solder_mask_margin 0.07))
    (pad 31 smd rect (at -1.77 -2.925 270) (size 0.85 0.28) (layers F.Cu F.Paste F.Mask)
      (net 104 "Net-(U2-Pad31)") (solder_mask_margin 0.07))
    (pad 30 smd rect (at -1.27 -2.925 270) (size 0.85 0.28) (layers F.Cu F.Paste F.Mask)
      (net 134 /DEBUG_RX) (solder_mask_margin 0.07))
    (pad 29 smd rect (at -0.77 -2.925 270) (size 0.85 0.28) (layers F.Cu F.Paste F.Mask)
      (net 105 "Net-(U2-Pad29)") (solder_mask_margin 0.07))
    (pad 28 smd rect (at -0.27 -2.925 270) (size 0.85 0.28) (layers F.Cu F.Paste F.Mask)
      (net 106 "Net-(U2-Pad28)") (solder_mask_margin 0.07))
    (pad 27 smd rect (at 0.23 -2.925 270) (size 0.85 0.28) (layers F.Cu F.Paste F.Mask)
      (net 107 "Net-(U2-Pad27)") (solder_mask_margin 0.07))
    (pad 26 smd rect (at 0.73 -2.925 270) (size 0.85 0.28) (layers F.Cu F.Paste F.Mask)
      (net 127 GND) (solder_mask_margin 0.07))
    (pad 24 smd rect (at 1.955 -2.2 270) (size 0.28 0.85) (layers F.Cu F.Paste F.Mask)
      (net 127 GND) (solder_mask_margin 0.07))
    (pad 23 smd rect (at 1.955 -1.7 270) (size 0.28 0.85) (layers F.Cu F.Paste F.Mask)
      (net 108 "Net-(U2-Pad23)") (solder_mask_margin 0.07))
    (pad 22 smd rect (at 1.955 -1.2 270) (size 0.28 0.85) (layers F.Cu F.Paste F.Mask)
      (net 109 "Net-(U2-Pad22)") (solder_mask_margin 0.07))
    (pad 21 smd rect (at 1.955 -0.7 270) (size 0.28 0.85) (layers F.Cu F.Paste F.Mask)
      (net 110 "Net-(U2-Pad21)") (solder_mask_margin 0.07))
    (pad 20 smd rect (at 1.955 -0.2 270) (size 0.28 0.85) (layers F.Cu F.Paste F.Mask)
      (net 127 GND) (solder_mask_margin 0.07))
    (pad 19 smd rect (at 1.955 0.3 270) (size 0.28 0.85) (layers F.Cu F.Paste F.Mask)
      (net 176 /s_USB_INTF.sch/FTDI_5V) (solder_mask_margin 0.07))
    (pad 18 smd rect (at 1.955 0.8 270) (size 0.28 0.85) (layers F.Cu F.Paste F.Mask)
      (net 111 "Net-(U2-Pad18)") (solder_mask_margin 0.07))
    (pad 16 smd rect (at 1.23 2.025 270) (size 0.85 0.28) (layers F.Cu F.Paste F.Mask)
      (net 177 /s_USB_INTF.sch/FTDI_3V3) (solder_mask_margin 0.07))
    (pad 15 smd rect (at 0.73 2.025 270) (size 0.85 0.28) (layers F.Cu F.Paste F.Mask)
      (net 130 /s_USB_INTF.sch/USB_D-) (solder_mask_margin 0.07))
    (pad 14 smd rect (at 0.23 2.025 270) (size 0.85 0.28) (layers F.Cu F.Paste F.Mask)
      (net 129 /s_USB_INTF.sch/USB_D+) (solder_mask_margin 0.07))
    (pad 13 smd rect (at -0.27 2.025 270) (size 0.85 0.28) (layers F.Cu F.Paste F.Mask)
      (net 112 "Net-(U2-Pad13)") (solder_mask_margin 0.07))
    (pad 12 smd rect (at -0.77 2.025 270) (size 0.85 0.28) (layers F.Cu F.Paste F.Mask)
      (net 113 "Net-(U2-Pad12)") (solder_mask_margin 0.07))
    (pad 11 smd rect (at -1.27 2.025 270) (size 0.85 0.28) (layers F.Cu F.Paste F.Mask)
      (net 114 "Net-(U2-Pad11)") (solder_mask_margin 0.07))
    (pad 10 smd rect (at -1.77 2.025 270) (size 0.85 0.28) (layers F.Cu F.Paste F.Mask)
      (net 115 "Net-(U2-Pad10)") (solder_mask_margin 0.07))
    (pad 8 smd rect (at -2.995 1.3 270) (size 0.28 0.85) (layers F.Cu F.Paste F.Mask)
      (net 116 "Net-(U2-Pad8)") (solder_mask_margin 0.07))
    (pad 7 smd rect (at -2.995 0.8 270) (size 0.28 0.85) (layers F.Cu F.Paste F.Mask)
      (net 117 "Net-(U2-Pad7)") (solder_mask_margin 0.07))
    (pad 6 smd rect (at -2.995 0.3 270) (size 0.28 0.85) (layers F.Cu F.Paste F.Mask)
      (net 118 "Net-(U2-Pad6)") (solder_mask_margin 0.07))
    (pad 5 smd rect (at -2.995 -0.2 270) (size 0.28 0.85) (layers F.Cu F.Paste F.Mask)
      (net 119 "Net-(U2-Pad5)") (solder_mask_margin 0.07))
    (pad 4 smd rect (at -2.995 -0.7 270) (size 0.28 0.85) (layers F.Cu F.Paste F.Mask)
      (net 127 GND) (solder_mask_margin 0.07))
    (pad 3 smd rect (at -2.995 -1.2 270) (size 0.28 0.85) (layers F.Cu F.Paste F.Mask)
      (net 120 "Net-(U2-Pad3)") (solder_mask_margin 0.07))
    (pad 2 smd rect (at -2.995 -1.7 270) (size 0.28 0.85) (layers F.Cu F.Paste F.Mask)
      (net 135 /DEBUG_TX) (solder_mask_margin 0.07))
    (pad 1 smd rect (at -2.995 -2.2 270) (size 0.28 0.85) (layers F.Cu F.Paste F.Mask)
      (net 177 /s_USB_INTF.sch/FTDI_3V3) (solder_mask_margin 0.07))
    (pad 33 thru_hole circle (at -1.52 0.55 270) (size 0.2 0.2) (drill 0.2) (layers *.Cu *.Mask)
      (net 127 GND) (solder_mask_margin 0.1))
    (pad 33 thru_hole circle (at -1.52 -0.45 270) (size 0.2 0.2) (drill 0.2) (layers *.Cu *.Mask)
      (net 127 GND) (solder_mask_margin 0.1))
    (pad 33 thru_hole circle (at -1.52 -1.45 270) (size 0.2 0.2) (drill 0.2) (layers *.Cu *.Mask)
      (net 127 GND) (solder_mask_margin 0.1))
    (pad 33 thru_hole circle (at -0.52 0.55 270) (size 0.2 0.2) (drill 0.2) (layers *.Cu *.Mask)
      (net 127 GND) (solder_mask_margin 0.1))
    (pad 33 thru_hole circle (at -0.52 -0.45 270) (size 0.2 0.2) (drill 0.2) (layers *.Cu *.Mask)
      (net 127 GND) (solder_mask_margin 0.1))
    (pad 33 thru_hole circle (at -0.52 -1.45 270) (size 0.2 0.2) (drill 0.2) (layers *.Cu *.Mask)
      (net 127 GND) (solder_mask_margin 0.1))
    (pad 33 thru_hole circle (at 0.48 0.55 270) (size 0.2 0.2) (drill 0.2) (layers *.Cu *.Mask)
      (net 127 GND) (solder_mask_margin 0.1))
    (pad 33 thru_hole circle (at 0.48 -0.45 270) (size 0.2 0.2) (drill 0.2) (layers *.Cu *.Mask)
      (net 127 GND) (solder_mask_margin 0.1))
    (pad 33 thru_hole circle (at 0.48 -1.45 270) (size 0.2 0.2) (drill 0.2) (layers *.Cu *.Mask)
      (net 127 GND) (solder_mask_margin 0.1))
    (pad 33 smd rect (at -0.52 -0.45 270) (size 3.45 3.45) (layers F.Cu F.Paste F.Mask)
      (net 127 GND))
    (pad 9 smd rect (at -2.27 2.025 270) (size 0.85 0.28) (layers F.Cu F.Paste F.Mask)
      (net 177 /s_USB_INTF.sch/FTDI_3V3) (solder_mask_margin 0.07))
    (pad 17 smd rect (at 1.955 1.3 270) (size 0.28 0.85) (layers F.Cu F.Paste F.Mask)
      (net 127 GND) (solder_mask_margin 0.07))
    (pad 25 smd rect (at 1.23 -2.925 270) (size 0.85 0.28) (layers F.Cu F.Paste F.Mask)
      (net 121 "Net-(U2-Pad25)") (solder_mask_margin 0.07))
  )

  (module penguin:QFP40P1600X1600X120-128N_ATSAME54P20A (layer F.Cu) (tedit 5E6D9777) (tstamp 5E752F71)
    (at 90.17 109.22 45)
    (path /5E7872D3/5E84F3B3)
    (fp_text reference U1 (at -4.500975 -9.803025 45) (layer F.SilkS)
      (effects (font (size 1.001331 1.001331) (thickness 0.015)))
    )
    (fp_text value p_ATSAME54P20A-AU (at 6.78639 10.114365 45) (layer F.Fab)
      (effects (font (size 1.002417 1.002417) (thickness 0.015)))
    )
    (fp_line (start -7 7) (end -7 6.6) (layer F.SilkS) (width 0.127))
    (fp_line (start -6.6 7) (end -7 7) (layer F.SilkS) (width 0.127))
    (fp_line (start 7 7) (end 7 6.6) (layer F.SilkS) (width 0.127))
    (fp_line (start 6.6 7) (end 7 7) (layer F.SilkS) (width 0.127))
    (fp_line (start 7 -7) (end 7 -6.6) (layer F.SilkS) (width 0.127))
    (fp_line (start 6.6 -7) (end 7 -7) (layer F.SilkS) (width 0.127))
    (fp_line (start -7 -7) (end -7 -6.6) (layer F.SilkS) (width 0.127))
    (fp_line (start -6.6 -7) (end -7 -7) (layer F.SilkS) (width 0.127))
    (fp_line (start 8.655 8.655) (end 8.655 -8.655) (layer F.CrtYd) (width 0.05))
    (fp_line (start -8.655 8.655) (end -8.655 -8.655) (layer F.CrtYd) (width 0.05))
    (fp_line (start -8.655 -8.655) (end 8.655 -8.655) (layer F.CrtYd) (width 0.05))
    (fp_line (start -8.655 8.655) (end 8.655 8.655) (layer F.CrtYd) (width 0.05))
    (fp_line (start -7 7) (end -7 -7) (layer F.Fab) (width 0.127))
    (fp_line (start 7 7) (end 7 -7) (layer F.Fab) (width 0.127))
    (fp_line (start 7 -7) (end -7 -7) (layer F.Fab) (width 0.127))
    (fp_line (start 7 7) (end -7 7) (layer F.Fab) (width 0.127))
    (fp_circle (center -9.14 -6.44) (end -8.94 -6.44) (layer F.Fab) (width 0.1))
    (fp_circle (center -9.14 -6.44) (end -8.94 -6.44) (layer F.SilkS) (width 0.1))
    (pad 96 smd rect (at 7.67 -6.2 45) (size 1.47 0.24) (layers F.Cu F.Paste F.Mask))
    (pad 95 smd rect (at 7.67 -5.8 45) (size 1.47 0.24) (layers F.Cu F.Paste F.Mask)
      (net 9 "Net-(U1-Pad95)"))
    (pad 94 smd rect (at 7.67 -5.4 45) (size 1.47 0.24) (layers F.Cu F.Paste F.Mask)
      (net 10 "Net-(U1-Pad94)"))
    (pad 93 smd rect (at 7.67 -5 45) (size 1.47 0.24) (layers F.Cu F.Paste F.Mask)
      (net 11 "Net-(U1-Pad93)"))
    (pad 92 smd rect (at 7.67 -4.6 45) (size 1.47 0.24) (layers F.Cu F.Paste F.Mask)
      (net 12 "Net-(U1-Pad92)"))
    (pad 91 smd rect (at 7.67 -4.2 45) (size 1.47 0.24) (layers F.Cu F.Paste F.Mask)
      (net 72 "Net-(U1-Pad107)"))
    (pad 90 smd rect (at 7.67 -3.8 45) (size 1.47 0.24) (layers F.Cu F.Paste F.Mask))
    (pad 89 smd rect (at 7.67 -3.4 45) (size 1.47 0.24) (layers F.Cu F.Paste F.Mask)
      (net 13 "Net-(U1-Pad89)"))
    (pad 88 smd rect (at 7.67 -3 45) (size 1.47 0.24) (layers F.Cu F.Paste F.Mask)
      (net 14 "Net-(U1-Pad88)"))
    (pad 87 smd rect (at 7.67 -2.6 45) (size 1.47 0.24) (layers F.Cu F.Paste F.Mask)
      (net 15 "Net-(U1-Pad87)"))
    (pad 86 smd rect (at 7.67 -2.2 45) (size 1.47 0.24) (layers F.Cu F.Paste F.Mask)
      (net 16 "Net-(U1-Pad86)"))
    (pad 85 smd rect (at 7.67 -1.8 45) (size 1.47 0.24) (layers F.Cu F.Paste F.Mask)
      (net 17 "Net-(U1-Pad85)"))
    (pad 84 smd rect (at 7.67 -1.4 45) (size 1.47 0.24) (layers F.Cu F.Paste F.Mask)
      (net 18 "Net-(U1-Pad84)"))
    (pad 83 smd rect (at 7.67 -1 45) (size 1.47 0.24) (layers F.Cu F.Paste F.Mask)
      (net 19 "Net-(U1-Pad83)"))
    (pad 82 smd rect (at 7.67 -0.6 45) (size 1.47 0.24) (layers F.Cu F.Paste F.Mask)
      (net 20 "Net-(U1-Pad82)"))
    (pad 81 smd rect (at 7.67 -0.2 45) (size 1.47 0.24) (layers F.Cu F.Paste F.Mask)
      (net 21 "Net-(U1-Pad81)"))
    (pad 80 smd rect (at 7.67 0.2 45) (size 1.47 0.24) (layers F.Cu F.Paste F.Mask)
      (net 22 "Net-(U1-Pad80)"))
    (pad 79 smd rect (at 7.67 0.6 45) (size 1.47 0.24) (layers F.Cu F.Paste F.Mask)
      (net 72 "Net-(U1-Pad107)"))
    (pad 78 smd rect (at 7.67 1 45) (size 1.47 0.24) (layers F.Cu F.Paste F.Mask))
    (pad 77 smd rect (at 7.67 1.4 45) (size 1.47 0.24) (layers F.Cu F.Paste F.Mask)
      (net 23 "Net-(U1-Pad77)"))
    (pad 76 smd rect (at 7.67 1.8 45) (size 1.47 0.24) (layers F.Cu F.Paste F.Mask)
      (net 24 "Net-(U1-Pad76)"))
    (pad 75 smd rect (at 7.67 2.2 45) (size 1.47 0.24) (layers F.Cu F.Paste F.Mask)
      (net 25 "Net-(U1-Pad75)"))
    (pad 74 smd rect (at 7.67 2.6 45) (size 1.47 0.24) (layers F.Cu F.Paste F.Mask)
      (net 26 "Net-(U1-Pad74)"))
    (pad 73 smd rect (at 7.67 3 45) (size 1.47 0.24) (layers F.Cu F.Paste F.Mask)
      (net 27 "Net-(U1-Pad73)"))
    (pad 72 smd rect (at 7.67 3.4 45) (size 1.47 0.24) (layers F.Cu F.Paste F.Mask)
      (net 28 "Net-(U1-Pad72)"))
    (pad 71 smd rect (at 7.67 3.8 45) (size 1.47 0.24) (layers F.Cu F.Paste F.Mask)
      (net 29 "Net-(U1-Pad71)"))
    (pad 70 smd rect (at 7.67 4.2 45) (size 1.47 0.24) (layers F.Cu F.Paste F.Mask)
      (net 30 "Net-(U1-Pad70)"))
    (pad 69 smd rect (at 7.67 4.6 45) (size 1.47 0.24) (layers F.Cu F.Paste F.Mask)
      (net 31 "Net-(U1-Pad69)"))
    (pad 68 smd rect (at 7.67 5 45) (size 1.47 0.24) (layers F.Cu F.Paste F.Mask)
      (net 32 "Net-(U1-Pad68)"))
    (pad 67 smd rect (at 7.67 5.4 45) (size 1.47 0.24) (layers F.Cu F.Paste F.Mask)
      (net 171 /MASTER_I2C_SCL))
    (pad 66 smd rect (at 7.67 5.8 45) (size 1.47 0.24) (layers F.Cu F.Paste F.Mask)
      (net 170 /MASTER_I2C_SDA))
    (pad 65 smd rect (at 7.67 6.2 45) (size 1.47 0.24) (layers F.Cu F.Paste F.Mask)
      (net 72 "Net-(U1-Pad107)"))
    (pad 32 smd rect (at -7.67 6.2 45) (size 1.47 0.24) (layers F.Cu F.Paste F.Mask)
      (net 33 "Net-(U1-Pad32)"))
    (pad 31 smd rect (at -7.67 5.8 45) (size 1.47 0.24) (layers F.Cu F.Paste F.Mask))
    (pad 30 smd rect (at -7.67 5.4 45) (size 1.47 0.24) (layers F.Cu F.Paste F.Mask)
      (net 34 "Net-(U1-Pad30)"))
    (pad 29 smd rect (at -7.67 5 45) (size 1.47 0.24) (layers F.Cu F.Paste F.Mask)
      (net 35 "Net-(U1-Pad29)"))
    (pad 28 smd rect (at -7.67 4.6 45) (size 1.47 0.24) (layers F.Cu F.Paste F.Mask)
      (net 36 "Net-(U1-Pad28)"))
    (pad 27 smd rect (at -7.67 4.2 45) (size 1.47 0.24) (layers F.Cu F.Paste F.Mask)
      (net 37 "Net-(U1-Pad27)"))
    (pad 26 smd rect (at -7.67 3.8 45) (size 1.47 0.24) (layers F.Cu F.Paste F.Mask)
      (net 38 "Net-(U1-Pad26)"))
    (pad 25 smd rect (at -7.67 3.4 45) (size 1.47 0.24) (layers F.Cu F.Paste F.Mask)
      (net 45 "Net-(U1-Pad14)"))
    (pad 24 smd rect (at -7.67 3 45) (size 1.47 0.24) (layers F.Cu F.Paste F.Mask)
      (net 39 "Net-(U1-Pad24)"))
    (pad 23 smd rect (at -7.67 2.6 45) (size 1.47 0.24) (layers F.Cu F.Paste F.Mask)
      (net 174 /MASTER_SPI_MISO))
    (pad 22 smd rect (at -7.67 2.2 45) (size 1.47 0.24) (layers F.Cu F.Paste F.Mask)
      (net 175 /MASTER_SPI_CLK))
    (pad 21 smd rect (at -7.67 1.8 45) (size 1.47 0.24) (layers F.Cu F.Paste F.Mask)
      (net 174 /MASTER_SPI_MISO))
    (pad 20 smd rect (at -7.67 1.4 45) (size 1.47 0.24) (layers F.Cu F.Paste F.Mask)
      (net 40 "Net-(U1-Pad20)"))
    (pad 19 smd rect (at -7.67 1 45) (size 1.47 0.24) (layers F.Cu F.Paste F.Mask)
      (net 41 "Net-(U1-Pad19)"))
    (pad 18 smd rect (at -7.67 0.6 45) (size 1.47 0.24) (layers F.Cu F.Paste F.Mask)
      (net 42 "Net-(U1-Pad18)"))
    (pad 17 smd rect (at -7.67 0.2 45) (size 1.47 0.24) (layers F.Cu F.Paste F.Mask)
      (net 190 /s_BRAIN/EXT_IRQ_5))
    (pad 16 smd rect (at -7.67 -0.2 45) (size 1.47 0.24) (layers F.Cu F.Paste F.Mask)
      (net 43 "Net-(U1-Pad16)"))
    (pad 15 smd rect (at -7.67 -0.6 45) (size 1.47 0.24) (layers F.Cu F.Paste F.Mask)
      (net 44 "Net-(U1-Pad15)"))
    (pad 14 smd rect (at -7.67 -1 45) (size 1.47 0.24) (layers F.Cu F.Paste F.Mask)
      (net 45 "Net-(U1-Pad14)"))
    (pad 13 smd rect (at -7.67 -1.4 45) (size 1.47 0.24) (layers F.Cu F.Paste F.Mask)
      (net 46 "Net-(U1-Pad13)"))
    (pad 12 smd rect (at -7.67 -1.8 45) (size 1.47 0.24) (layers F.Cu F.Paste F.Mask)
      (net 191 /s_BRAIN/EXT_IRQ_4))
    (pad 11 smd rect (at -7.67 -2.2 45) (size 1.47 0.24) (layers F.Cu F.Paste F.Mask)
      (net 192 /s_BRAIN/EXT_IRQ_3))
    (pad 10 smd rect (at -7.67 -2.6 45) (size 1.47 0.24) (layers F.Cu F.Paste F.Mask)
      (net 47 "Net-(U1-Pad10)"))
    (pad 9 smd rect (at -7.67 -3 45) (size 1.47 0.24) (layers F.Cu F.Paste F.Mask)
      (net 48 "Net-(U1-Pad9)"))
    (pad 8 smd rect (at -7.67 -3.4 45) (size 1.47 0.24) (layers F.Cu F.Paste F.Mask)
      (net 49 "Net-(U1-Pad8)"))
    (pad 7 smd rect (at -7.67 -3.8 45) (size 1.47 0.24) (layers F.Cu F.Paste F.Mask)
      (net 50 "Net-(U1-Pad7)"))
    (pad 6 smd rect (at -7.67 -4.2 45) (size 1.47 0.24) (layers F.Cu F.Paste F.Mask)
      (net 51 "Net-(U1-Pad6)"))
    (pad 5 smd rect (at -7.67 -4.6 45) (size 1.47 0.24) (layers F.Cu F.Paste F.Mask)
      (net 52 "Net-(U1-Pad5)"))
    (pad 4 smd rect (at -7.67 -5 45) (size 1.47 0.24) (layers F.Cu F.Paste F.Mask)
      (net 53 "Net-(U1-Pad4)"))
    (pad 3 smd rect (at -7.67 -5.4 45) (size 1.47 0.24) (layers F.Cu F.Paste F.Mask)
      (net 54 "Net-(U1-Pad3)"))
    (pad 2 smd rect (at -7.67 -5.8 45) (size 1.47 0.24) (layers F.Cu F.Paste F.Mask)
      (net 131 "Net-(C2-Pad1)"))
    (pad 1 smd rect (at -7.67 -6.2 45) (size 1.47 0.24) (layers F.Cu F.Paste F.Mask)
      (net 55 "Net-(C1-Pad2)"))
    (pad 128 smd rect (at -6.2 -7.67 45) (size 0.24 1.47) (layers F.Cu F.Paste F.Mask)
      (net 122 g_3v3))
    (pad 127 smd rect (at -5.8 -7.67 45) (size 0.24 1.47) (layers F.Cu F.Paste F.Mask)
      (net 193 /s_BRAIN/EXT_IRQ_2))
    (pad 126 smd rect (at -5.4 -7.67 45) (size 0.24 1.47) (layers F.Cu F.Paste F.Mask)
      (net 194 /s_BRAIN/EXT_IRQ_1))
    (pad 125 smd rect (at -5 -7.67 45) (size 0.24 1.47) (layers F.Cu F.Paste F.Mask)
      (net 195 /s_BRAIN/EXT_IRQ_0))
    (pad 124 smd rect (at -4.6 -7.67 45) (size 0.24 1.47) (layers F.Cu F.Paste F.Mask)
      (net 56 "Net-(U1-Pad124)"))
    (pad 123 smd rect (at -4.2 -7.67 45) (size 0.24 1.47) (layers F.Cu F.Paste F.Mask)
      (net 57 "Net-(U1-Pad123)"))
    (pad 122 smd rect (at -3.8 -7.67 45) (size 0.24 1.47) (layers F.Cu F.Paste F.Mask)
      (net 58 "Net-(U1-Pad122)"))
    (pad 121 smd rect (at -3.4 -7.67 45) (size 0.24 1.47) (layers F.Cu F.Paste F.Mask)
      (net 59 "Net-(U1-Pad121)"))
    (pad 120 smd rect (at -3 -7.67 45) (size 0.24 1.47) (layers F.Cu F.Paste F.Mask)
      (net 60 "Net-(U1-Pad120)"))
    (pad 119 smd rect (at -2.6 -7.67 45) (size 0.24 1.47) (layers F.Cu F.Paste F.Mask)
      (net 61 "Net-(U1-Pad119)"))
    (pad 118 smd rect (at -2.2 -7.67 45) (size 0.24 1.47) (layers F.Cu F.Paste F.Mask)
      (net 72 "Net-(U1-Pad107)"))
    (pad 117 smd rect (at -1.8 -7.67 45) (size 0.24 1.47) (layers F.Cu F.Paste F.Mask)
      (net 62 "Net-(U1-Pad117)"))
    (pad 116 smd rect (at -1.4 -7.67 45) (size 0.24 1.47) (layers F.Cu F.Paste F.Mask)
      (net 63 "Net-(U1-Pad116)"))
    (pad 115 smd rect (at -1 -7.67 45) (size 0.24 1.47) (layers F.Cu F.Paste F.Mask)
      (net 64 "Net-(U1-Pad115)"))
    (pad 114 smd rect (at -0.6 -7.67 45) (size 0.24 1.47) (layers F.Cu F.Paste F.Mask)
      (net 65 "Net-(U1-Pad114)"))
    (pad 113 smd rect (at -0.2 -7.67 45) (size 0.24 1.47) (layers F.Cu F.Paste F.Mask)
      (net 66 "Net-(U1-Pad113)"))
    (pad 112 smd rect (at 0.2 -7.67 45) (size 0.24 1.47) (layers F.Cu F.Paste F.Mask)
      (net 67 "Net-(U1-Pad112)"))
    (pad 111 smd rect (at 0.6 -7.67 45) (size 0.24 1.47) (layers F.Cu F.Paste F.Mask)
      (net 68 "Net-(U1-Pad111)"))
    (pad 110 smd rect (at 1 -7.67 45) (size 0.24 1.47) (layers F.Cu F.Paste F.Mask)
      (net 69 "Net-(U1-Pad110)"))
    (pad 109 smd rect (at 1.4 -7.67 45) (size 0.24 1.47) (layers F.Cu F.Paste F.Mask)
      (net 70 "Net-(U1-Pad109)"))
    (pad 108 smd rect (at 1.8 -7.67 45) (size 0.24 1.47) (layers F.Cu F.Paste F.Mask)
      (net 71 "Net-(U1-Pad108)"))
    (pad 107 smd rect (at 2.2 -7.67 45) (size 0.24 1.47) (layers F.Cu F.Paste F.Mask)
      (net 72 "Net-(U1-Pad107)"))
    (pad 106 smd rect (at 2.6 -7.67 45) (size 0.24 1.47) (layers F.Cu F.Paste F.Mask))
    (pad 105 smd rect (at 3 -7.67 45) (size 0.24 1.47) (layers F.Cu F.Paste F.Mask)
      (net 73 "Net-(U1-Pad105)"))
    (pad 104 smd rect (at 3.4 -7.67 45) (size 0.24 1.47) (layers F.Cu F.Paste F.Mask)
      (net 74 "Net-(U1-Pad104)"))
    (pad 103 smd rect (at 3.8 -7.67 45) (size 0.24 1.47) (layers F.Cu F.Paste F.Mask)
      (net 75 "Net-(U1-Pad103)"))
    (pad 102 smd rect (at 4.2 -7.67 45) (size 0.24 1.47) (layers F.Cu F.Paste F.Mask)
      (net 76 "Net-(U1-Pad102)"))
    (pad 101 smd rect (at 4.6 -7.67 45) (size 0.24 1.47) (layers F.Cu F.Paste F.Mask)
      (net 135 /DEBUG_TX))
    (pad 100 smd rect (at 5 -7.67 45) (size 0.24 1.47) (layers F.Cu F.Paste F.Mask)
      (net 134 /DEBUG_RX))
    (pad 99 smd rect (at 5.4 -7.67 45) (size 0.24 1.47) (layers F.Cu F.Paste F.Mask)
      (net 77 "Net-(U1-Pad99)"))
    (pad 98 smd rect (at 5.8 -7.67 45) (size 0.24 1.47) (layers F.Cu F.Paste F.Mask)
      (net 78 "Net-(U1-Pad98)"))
    (pad 97 smd rect (at 6.2 -7.67 45) (size 0.24 1.47) (layers F.Cu F.Paste F.Mask)
      (net 72 "Net-(U1-Pad107)"))
    (pad 64 smd rect (at 6.2 7.67 45) (size 0.24 1.47) (layers F.Cu F.Paste F.Mask))
    (pad 63 smd rect (at 5.8 7.67 45) (size 0.24 1.47) (layers F.Cu F.Paste F.Mask)
      (net 132 "Net-(C5-Pad2)"))
    (pad 62 smd rect (at 5.4 7.67 45) (size 0.24 1.47) (layers F.Cu F.Paste F.Mask)
      (net 133 "Net-(C4-Pad2)"))
    (pad 61 smd rect (at 5 7.67 45) (size 0.24 1.47) (layers F.Cu F.Paste F.Mask)
      (net 79 "Net-(U1-Pad61)"))
    (pad 60 smd rect (at 4.6 7.67 45) (size 0.24 1.47) (layers F.Cu F.Paste F.Mask)
      (net 80 "Net-(U1-Pad60)"))
    (pad 59 smd rect (at 4.2 7.67 45) (size 0.24 1.47) (layers F.Cu F.Paste F.Mask)
      (net 81 "Net-(U1-Pad59)"))
    (pad 58 smd rect (at 3.8 7.67 45) (size 0.24 1.47) (layers F.Cu F.Paste F.Mask)
      (net 82 "Net-(U1-Pad58)"))
    (pad 57 smd rect (at 3.4 7.67 45) (size 0.24 1.47) (layers F.Cu F.Paste F.Mask)
      (net 83 "Net-(U1-Pad57)"))
    (pad 56 smd rect (at 3 7.67 45) (size 0.24 1.47) (layers F.Cu F.Paste F.Mask)
      (net 84 "Net-(U1-Pad56)"))
    (pad 55 smd rect (at 2.6 7.67 45) (size 0.24 1.47) (layers F.Cu F.Paste F.Mask)
      (net 85 "Net-(U1-Pad55)"))
    (pad 54 smd rect (at 2.2 7.67 45) (size 0.24 1.47) (layers F.Cu F.Paste F.Mask)
      (net 72 "Net-(U1-Pad107)"))
    (pad 53 smd rect (at 1.8 7.67 45) (size 0.24 1.47) (layers F.Cu F.Paste F.Mask))
    (pad 52 smd rect (at 1.4 7.67 45) (size 0.24 1.47) (layers F.Cu F.Paste F.Mask)
      (net 86 "Net-(U1-Pad52)"))
    (pad 51 smd rect (at 1 7.67 45) (size 0.24 1.47) (layers F.Cu F.Paste F.Mask)
      (net 87 "Net-(U1-Pad51)"))
    (pad 50 smd rect (at 0.6 7.67 45) (size 0.24 1.47) (layers F.Cu F.Paste F.Mask)
      (net 88 "Net-(U1-Pad50)"))
    (pad 49 smd rect (at 0.2 7.67 45) (size 0.24 1.47) (layers F.Cu F.Paste F.Mask)
      (net 89 "Net-(U1-Pad49)"))
    (pad 48 smd rect (at -0.2 7.67 45) (size 0.24 1.47) (layers F.Cu F.Paste F.Mask)
      (net 90 "Net-(U1-Pad48)"))
    (pad 47 smd rect (at -0.6 7.67 45) (size 0.24 1.47) (layers F.Cu F.Paste F.Mask)
      (net 91 "Net-(U1-Pad47)"))
    (pad 46 smd rect (at -1 7.67 45) (size 0.24 1.47) (layers F.Cu F.Paste F.Mask)
      (net 72 "Net-(U1-Pad107)"))
    (pad 45 smd rect (at -1.4 7.67 45) (size 0.24 1.47) (layers F.Cu F.Paste F.Mask))
    (pad 44 smd rect (at -1.8 7.67 45) (size 0.24 1.47) (layers F.Cu F.Paste F.Mask)
      (net 92 "Net-(U1-Pad44)"))
    (pad 43 smd rect (at -2.2 7.67 45) (size 0.24 1.47) (layers F.Cu F.Paste F.Mask)
      (net 93 "Net-(U1-Pad43)"))
    (pad 42 smd rect (at -2.6 7.67 45) (size 0.24 1.47) (layers F.Cu F.Paste F.Mask)
      (net 94 "Net-(U1-Pad42)"))
    (pad 41 smd rect (at -3 7.67 45) (size 0.24 1.47) (layers F.Cu F.Paste F.Mask)
      (net 95 "Net-(U1-Pad41)"))
    (pad 40 smd rect (at -3.4 7.67 45) (size 0.24 1.47) (layers F.Cu F.Paste F.Mask)
      (net 96 "Net-(U1-Pad40)"))
    (pad 39 smd rect (at -3.8 7.67 45) (size 0.24 1.47) (layers F.Cu F.Paste F.Mask)
      (net 97 "Net-(U1-Pad39)"))
    (pad 38 smd rect (at -4.2 7.67 45) (size 0.24 1.47) (layers F.Cu F.Paste F.Mask))
    (pad 37 smd rect (at -4.6 7.67 45) (size 0.24 1.47) (layers F.Cu F.Paste F.Mask)
      (net 98 "Net-(U1-Pad37)"))
    (pad 36 smd rect (at -5 7.67 45) (size 0.24 1.47) (layers F.Cu F.Paste F.Mask)
      (net 99 "Net-(U1-Pad36)"))
    (pad 35 smd rect (at -5.4 7.67 45) (size 0.24 1.47) (layers F.Cu F.Paste F.Mask)
      (net 100 "Net-(U1-Pad35)"))
    (pad 34 smd rect (at -5.8 7.67 45) (size 0.24 1.47) (layers F.Cu F.Paste F.Mask)
      (net 101 "Net-(U1-Pad34)"))
    (pad 33 smd rect (at -6.2 7.67 45) (size 0.24 1.47) (layers F.Cu F.Paste F.Mask)
      (net 102 "Net-(U1-Pad33)"))
  )

  (module Connector_IDC:IDC-Header_2x20_P2.54mm_Horizontal (layer F.Cu) (tedit 59DE239E) (tstamp 5E752EDB)
    (at 78.74 64.77 90)
    (descr "Through hole angled IDC box header, 2x20, 2.54mm pitch, double rows")
    (tags "Through hole IDC box header THT 2x20 2.54mm double row")
    (path /5E8589A7/5E858ED6)
    (fp_text reference J3 (at 6.105 -6.35 90) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value Conn_02x20_Odd_Even_LCD_INTF (at 6.105 54.864 90) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start 13.48 53.61) (end -1.12 53.61) (layer F.CrtYd) (width 0.05))
    (fp_line (start 13.48 -5.35) (end 13.48 53.61) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.12 53.61) (end -1.12 -5.35) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.12 -5.35) (end 13.48 -5.35) (layer F.CrtYd) (width 0.05))
    (fp_line (start 4.13 53.61) (end 4.13 -5.35) (layer F.SilkS) (width 0.12))
    (fp_line (start 4.13 53.61) (end 13.48 53.61) (layer F.SilkS) (width 0.12))
    (fp_line (start 4.13 26.38) (end 13.48 26.38) (layer F.SilkS) (width 0.12))
    (fp_line (start 4.13 21.88) (end 13.48 21.88) (layer F.SilkS) (width 0.12))
    (fp_line (start 4.13 -5.35) (end 13.48 -5.35) (layer F.SilkS) (width 0.12))
    (fp_line (start 13.48 -5.35) (end 13.48 53.61) (layer F.SilkS) (width 0.12))
    (fp_line (start 0 -1.27) (end -1.27 -1.27) (layer F.SilkS) (width 0.12))
    (fp_line (start -1.27 -1.27) (end -1.27 0) (layer F.SilkS) (width 0.12))
    (fp_line (start 5.38 -5.1) (end 13.23 -5.1) (layer F.Fab) (width 0.1))
    (fp_line (start 4.38 9.84) (end -0.32 9.84) (layer F.Fab) (width 0.1))
    (fp_line (start 4.38 7.3) (end -0.32 7.3) (layer F.Fab) (width 0.1))
    (fp_line (start 4.38 53.36) (end 4.38 -4.1) (layer F.Fab) (width 0.1))
    (fp_line (start 4.38 53.36) (end 13.23 53.36) (layer F.Fab) (width 0.1))
    (fp_line (start 4.38 47.94) (end -0.32 47.94) (layer F.Fab) (width 0.1))
    (fp_line (start 4.38 45.4) (end -0.32 45.4) (layer F.Fab) (width 0.1))
    (fp_line (start 4.38 42.86) (end -0.32 42.86) (layer F.Fab) (width 0.1))
    (fp_line (start 4.38 40.32) (end -0.32 40.32) (layer F.Fab) (width 0.1))
    (fp_line (start 4.38 4.76) (end -0.32 4.76) (layer F.Fab) (width 0.1))
    (fp_line (start 4.38 37.78) (end -0.32 37.78) (layer F.Fab) (width 0.1))
    (fp_line (start 4.38 35.24) (end -0.32 35.24) (layer F.Fab) (width 0.1))
    (fp_line (start 4.38 32.7) (end -0.32 32.7) (layer F.Fab) (width 0.1))
    (fp_line (start 4.38 30.16) (end -0.32 30.16) (layer F.Fab) (width 0.1))
    (fp_line (start 4.38 27.62) (end -0.32 27.62) (layer F.Fab) (width 0.1))
    (fp_line (start 4.38 26.38) (end 13.23 26.38) (layer F.Fab) (width 0.1))
    (fp_line (start 4.38 25.08) (end -0.32 25.08) (layer F.Fab) (width 0.1))
    (fp_line (start 4.38 22.54) (end -0.32 22.54) (layer F.Fab) (width 0.1))
    (fp_line (start 4.38 21.88) (end 13.23 21.88) (layer F.Fab) (width 0.1))
    (fp_line (start 4.38 20) (end -0.32 20) (layer F.Fab) (width 0.1))
    (fp_line (start 4.38 2.22) (end -0.32 2.22) (layer F.Fab) (width 0.1))
    (fp_line (start 4.38 17.46) (end -0.32 17.46) (layer F.Fab) (width 0.1))
    (fp_line (start 4.38 14.92) (end -0.32 14.92) (layer F.Fab) (width 0.1))
    (fp_line (start 4.38 12.38) (end -0.32 12.38) (layer F.Fab) (width 0.1))
    (fp_line (start 4.38 -4.1) (end 5.38 -5.1) (layer F.Fab) (width 0.1))
    (fp_line (start 4.38 -0.32) (end -0.32 -0.32) (layer F.Fab) (width 0.1))
    (fp_line (start 13.23 53.36) (end 13.23 -5.1) (layer F.Fab) (width 0.1))
    (fp_line (start -0.32 9.84) (end -0.32 10.48) (layer F.Fab) (width 0.1))
    (fp_line (start -0.32 7.94) (end 4.38 7.94) (layer F.Fab) (width 0.1))
    (fp_line (start -0.32 7.3) (end -0.32 7.94) (layer F.Fab) (width 0.1))
    (fp_line (start -0.32 5.4) (end 4.38 5.4) (layer F.Fab) (width 0.1))
    (fp_line (start -0.32 48.58) (end 4.38 48.58) (layer F.Fab) (width 0.1))
    (fp_line (start -0.32 47.94) (end -0.32 48.58) (layer F.Fab) (width 0.1))
    (fp_line (start -0.32 46.04) (end 4.38 46.04) (layer F.Fab) (width 0.1))
    (fp_line (start -0.32 45.4) (end -0.32 46.04) (layer F.Fab) (width 0.1))
    (fp_line (start -0.32 43.5) (end 4.38 43.5) (layer F.Fab) (width 0.1))
    (fp_line (start -0.32 42.86) (end -0.32 43.5) (layer F.Fab) (width 0.1))
    (fp_line (start -0.32 40.96) (end 4.38 40.96) (layer F.Fab) (width 0.1))
    (fp_line (start -0.32 40.32) (end -0.32 40.96) (layer F.Fab) (width 0.1))
    (fp_line (start -0.32 4.76) (end -0.32 5.4) (layer F.Fab) (width 0.1))
    (fp_line (start -0.32 38.42) (end 4.38 38.42) (layer F.Fab) (width 0.1))
    (fp_line (start -0.32 37.78) (end -0.32 38.42) (layer F.Fab) (width 0.1))
    (fp_line (start -0.32 35.88) (end 4.38 35.88) (layer F.Fab) (width 0.1))
    (fp_line (start -0.32 35.24) (end -0.32 35.88) (layer F.Fab) (width 0.1))
    (fp_line (start -0.32 33.34) (end 4.38 33.34) (layer F.Fab) (width 0.1))
    (fp_line (start -0.32 32.7) (end -0.32 33.34) (layer F.Fab) (width 0.1))
    (fp_line (start -0.32 30.8) (end 4.38 30.8) (layer F.Fab) (width 0.1))
    (fp_line (start -0.32 30.16) (end -0.32 30.8) (layer F.Fab) (width 0.1))
    (fp_line (start -0.32 28.26) (end 4.38 28.26) (layer F.Fab) (width 0.1))
    (fp_line (start -0.32 27.62) (end -0.32 28.26) (layer F.Fab) (width 0.1))
    (fp_line (start -0.32 25.72) (end 4.38 25.72) (layer F.Fab) (width 0.1))
    (fp_line (start -0.32 25.08) (end -0.32 25.72) (layer F.Fab) (width 0.1))
    (fp_line (start -0.32 23.18) (end 4.38 23.18) (layer F.Fab) (width 0.1))
    (fp_line (start -0.32 22.54) (end -0.32 23.18) (layer F.Fab) (width 0.1))
    (fp_line (start -0.32 20.64) (end 4.38 20.64) (layer F.Fab) (width 0.1))
    (fp_line (start -0.32 20) (end -0.32 20.64) (layer F.Fab) (width 0.1))
    (fp_line (start -0.32 2.86) (end 4.38 2.86) (layer F.Fab) (width 0.1))
    (fp_line (start -0.32 2.22) (end -0.32 2.86) (layer F.Fab) (width 0.1))
    (fp_line (start -0.32 18.1) (end 4.38 18.1) (layer F.Fab) (width 0.1))
    (fp_line (start -0.32 17.46) (end -0.32 18.1) (layer F.Fab) (width 0.1))
    (fp_line (start -0.32 15.56) (end 4.38 15.56) (layer F.Fab) (width 0.1))
    (fp_line (start -0.32 14.92) (end -0.32 15.56) (layer F.Fab) (width 0.1))
    (fp_line (start -0.32 13.02) (end 4.38 13.02) (layer F.Fab) (width 0.1))
    (fp_line (start -0.32 12.38) (end -0.32 13.02) (layer F.Fab) (width 0.1))
    (fp_line (start -0.32 10.48) (end 4.38 10.48) (layer F.Fab) (width 0.1))
    (fp_line (start -0.32 0.32) (end 4.38 0.32) (layer F.Fab) (width 0.1))
    (fp_line (start -0.32 -0.32) (end -0.32 0.32) (layer F.Fab) (width 0.1))
    (fp_text user %R (at 8.805 24.13) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (pad 40 thru_hole oval (at 2.54 48.26 90) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 5 "Net-(J3-Pad40)"))
    (pad 39 thru_hole oval (at 0 48.26 90) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 6 "Net-(J3-Pad39)"))
    (pad 38 thru_hole oval (at 2.54 45.72 90) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 7 "Net-(J3-Pad38)"))
    (pad 37 thru_hole oval (at 0 45.72 90) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 136 /s_SCREEN_INTF/TFT_STB))
    (pad 36 thru_hole oval (at 2.54 43.18 90) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 137 /s_SCREEN_INTF/D23))
    (pad 35 thru_hole oval (at 0 43.18 90) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 138 /s_SCREEN_INTF/D22))
    (pad 34 thru_hole oval (at 2.54 40.64 90) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 139 /s_SCREEN_INTF/D21))
    (pad 33 thru_hole oval (at 0 40.64 90) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 140 /s_SCREEN_INTF/D20))
    (pad 32 thru_hole oval (at 2.54 38.1 90) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 141 /s_SCREEN_INTF/D19))
    (pad 31 thru_hole oval (at 0 38.1 90) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 142 /s_SCREEN_INTF/D18))
    (pad 30 thru_hole oval (at 2.54 35.56 90) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 143 /s_SCREEN_INTF/D17))
    (pad 29 thru_hole oval (at 0 35.56 90) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 144 /s_SCREEN_INTF/D16))
    (pad 28 thru_hole oval (at 2.54 33.02 90) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 145 /s_SCREEN_INTF/D15))
    (pad 27 thru_hole oval (at 0 33.02 90) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 146 /s_SCREEN_INTF/D14))
    (pad 26 thru_hole oval (at 2.54 30.48 90) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 147 /s_SCREEN_INTF/D13))
    (pad 25 thru_hole oval (at 0 30.48 90) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 148 /s_SCREEN_INTF/D12))
    (pad 24 thru_hole oval (at 2.54 27.94 90) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 149 /s_SCREEN_INTF/D11))
    (pad 23 thru_hole oval (at 0 27.94 90) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 150 /s_SCREEN_INTF/D10))
    (pad 22 thru_hole oval (at 2.54 25.4 90) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 151 /s_SCREEN_INTF/D9))
    (pad 21 thru_hole oval (at 0 25.4 90) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 152 /s_SCREEN_INTF/D8))
    (pad 20 thru_hole oval (at 2.54 22.86 90) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 153 /s_SCREEN_INTF/D7))
    (pad 19 thru_hole oval (at 0 22.86 90) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 154 /s_SCREEN_INTF/D6))
    (pad 18 thru_hole oval (at 2.54 20.32 90) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 155 /s_SCREEN_INTF/D5))
    (pad 17 thru_hole oval (at 0 20.32 90) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 156 /s_SCREEN_INTF/D4))
    (pad 16 thru_hole oval (at 2.54 17.78 90) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 157 /s_SCREEN_INTF/D3))
    (pad 15 thru_hole oval (at 0 17.78 90) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 158 /s_SCREEN_INTF/D2))
    (pad 14 thru_hole oval (at 2.54 15.24 90) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 159 /s_SCREEN_INTF/D1))
    (pad 13 thru_hole oval (at 0 15.24 90) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 160 /s_SCREEN_INTF/D0))
    (pad 12 thru_hole oval (at 2.54 12.7 90) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 161 /s_SCREEN_INTF/TFT_TE))
    (pad 11 thru_hole oval (at 0 12.7 90) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 162 /s_SCREEN_INTF/~TFT_RD))
    (pad 10 thru_hole oval (at 2.54 10.16 90) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 163 /s_SCREEN_INTF/~TFT_WR))
    (pad 9 thru_hole oval (at 0 10.16 90) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 169 /~TFT_CS))
    (pad 8 thru_hole oval (at 2.54 7.62 90) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 164 /s_SCREEN_INTF/TFT_RSDC))
    (pad 7 thru_hole oval (at 0 7.62 90) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 165 /s_SCREEN_INTF/~TFT_RST))
    (pad 6 thru_hole oval (at 2.54 5.08 90) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 8 "Net-(J3-Pad6)"))
    (pad 5 thru_hole oval (at 0 5.08 90) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 166 /s_SCREEN_INTF/TFT_TOUCH_INT))
    (pad 4 thru_hole oval (at 2.54 2.54 90) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 170 /MASTER_I2C_SDA))
    (pad 3 thru_hole oval (at 0 2.54 90) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 171 /MASTER_I2C_SCL))
    (pad 2 thru_hole oval (at 2.54 0 90) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 127 GND))
    (pad 1 thru_hole rect (at 0 0 90) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 122 g_3v3))
    (model ${KISYS3DMOD}/Connector_IDC.3dshapes/IDC-Header_2x20_P2.54mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Connector_USB:USB_Micro-B_Wuerth_629105150521 (layer F.Cu) (tedit 5A142044) (tstamp 5E752E24)
    (at 54.61 73.66 270)
    (descr "USB Micro-B receptacle, http://www.mouser.com/ds/2/445/629105150521-469306.pdf")
    (tags "usb micro receptacle")
    (path /5E7C0F59/5E8480AD)
    (attr smd)
    (fp_text reference J1 (at 0 -3.5 90) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value USB_B_Micro (at 0 5.6 90) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text user "PCB Edge" (at 0 3.75 90) (layer Dwgs.User)
      (effects (font (size 0.5 0.5) (thickness 0.08)))
    )
    (fp_text user %R (at 0 1.05 90) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start 4.95 -3.34) (end -4.94 -3.34) (layer F.CrtYd) (width 0.05))
    (fp_line (start 4.95 4.85) (end 4.95 -3.34) (layer F.CrtYd) (width 0.05))
    (fp_line (start -4.94 4.85) (end 4.95 4.85) (layer F.CrtYd) (width 0.05))
    (fp_line (start -4.94 -3.34) (end -4.94 4.85) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.8 -2.4) (end 2.8 -2.4) (layer F.SilkS) (width 0.15))
    (fp_line (start -1.8 -2.4) (end -2.8 -2.4) (layer F.SilkS) (width 0.15))
    (fp_line (start -1.8 -2.825) (end -1.8 -2.4) (layer F.SilkS) (width 0.15))
    (fp_line (start -1.075 -2.825) (end -1.8 -2.825) (layer F.SilkS) (width 0.15))
    (fp_line (start 4.15 0.75) (end 4.15 -0.65) (layer F.SilkS) (width 0.15))
    (fp_line (start 4.15 3.3) (end 4.15 3.15) (layer F.SilkS) (width 0.15))
    (fp_line (start 3.85 3.3) (end 4.15 3.3) (layer F.SilkS) (width 0.15))
    (fp_line (start 3.85 3.75) (end 3.85 3.3) (layer F.SilkS) (width 0.15))
    (fp_line (start -3.85 3.3) (end -3.85 3.75) (layer F.SilkS) (width 0.15))
    (fp_line (start -4.15 3.3) (end -3.85 3.3) (layer F.SilkS) (width 0.15))
    (fp_line (start -4.15 3.15) (end -4.15 3.3) (layer F.SilkS) (width 0.15))
    (fp_line (start -4.15 -0.65) (end -4.15 0.75) (layer F.SilkS) (width 0.15))
    (fp_line (start -1.075 -2.95) (end -1.075 -2.725) (layer F.Fab) (width 0.15))
    (fp_line (start -1.525 -2.95) (end -1.075 -2.95) (layer F.Fab) (width 0.15))
    (fp_line (start -1.525 -2.725) (end -1.525 -2.95) (layer F.Fab) (width 0.15))
    (fp_line (start -1.3 -2.55) (end -1.525 -2.725) (layer F.Fab) (width 0.15))
    (fp_line (start -1.075 -2.725) (end -1.3 -2.55) (layer F.Fab) (width 0.15))
    (fp_line (start -2.7 3.75) (end 2.7 3.75) (layer F.Fab) (width 0.15))
    (fp_line (start 4 -2.25) (end -4 -2.25) (layer F.Fab) (width 0.15))
    (fp_line (start 4 3.15) (end 4 -2.25) (layer F.Fab) (width 0.15))
    (fp_line (start 3.7 3.15) (end 4 3.15) (layer F.Fab) (width 0.15))
    (fp_line (start 3.7 4.35) (end 3.7 3.15) (layer F.Fab) (width 0.15))
    (fp_line (start -3.7 4.35) (end 3.7 4.35) (layer F.Fab) (width 0.15))
    (fp_line (start -3.7 3.15) (end -3.7 4.35) (layer F.Fab) (width 0.15))
    (fp_line (start -4 3.15) (end -3.7 3.15) (layer F.Fab) (width 0.15))
    (fp_line (start -4 -2.25) (end -4 3.15) (layer F.Fab) (width 0.15))
    (pad "" np_thru_hole oval (at 2.5 -0.8 270) (size 0.8 0.8) (drill 0.8) (layers *.Cu *.Mask))
    (pad "" np_thru_hole oval (at -2.5 -0.8 270) (size 0.8 0.8) (drill 0.8) (layers *.Cu *.Mask))
    (pad 6 thru_hole oval (at 3.875 1.95 270) (size 1.15 1.8) (drill oval 0.55 1.2) (layers *.Cu *.Mask)
      (net 127 GND))
    (pad 6 thru_hole oval (at -3.875 1.95 270) (size 1.15 1.8) (drill oval 0.55 1.2) (layers *.Cu *.Mask)
      (net 127 GND))
    (pad 6 thru_hole oval (at 3.725 -1.85 270) (size 1.45 2) (drill oval 0.85 1.4) (layers *.Cu *.Mask)
      (net 127 GND))
    (pad 6 thru_hole oval (at -3.725 -1.85 270) (size 1.45 2) (drill oval 0.85 1.4) (layers *.Cu *.Mask)
      (net 127 GND))
    (pad 5 smd rect (at 1.3 -1.9 270) (size 0.45 1.3) (layers F.Cu F.Paste F.Mask)
      (net 127 GND))
    (pad 4 smd rect (at 0.65 -1.9 270) (size 0.45 1.3) (layers F.Cu F.Paste F.Mask)
      (net 1 "Net-(J1-Pad4)"))
    (pad 3 smd rect (at 0 -1.9 270) (size 0.45 1.3) (layers F.Cu F.Paste F.Mask)
      (net 129 /s_USB_INTF.sch/USB_D+))
    (pad 2 smd rect (at -0.65 -1.9 270) (size 0.45 1.3) (layers F.Cu F.Paste F.Mask)
      (net 130 /s_USB_INTF.sch/USB_D-))
    (pad 1 smd rect (at -1.3 -1.9 270) (size 0.45 1.3) (layers F.Cu F.Paste F.Mask)
      (net 168 "Net-(C7-Pad1)"))
    (model ${KISYS3DMOD}/Connector_USB.3dshapes/USB_Micro-B_Wuerth_629105150521.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (gr_line (start 50.8 130.81) (end 50.8 50.8) (layer Edge.Cuts) (width 0.05) (tstamp 5E7ADE31))
  (gr_line (start 152.4 130.81) (end 50.8 130.81) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 152.4 50.8) (end 152.4 130.81) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 53.34 50.8) (end 152.4 50.8) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 50.8 50.8) (end 53.34 50.8) (layer Edge.Cuts) (width 0.05) (tstamp 5E6E9EBC))

)
