format_version: '2'
name: SPI_SD_MMC_Lib
versions:
  api: '1.0'
  backend: 1.8.472
  commit: 605bd5a7663644fb84783aa2b00942b79b0d8955
  content: unknown
  content_pack_name: unknown
  format: '2'
  frontend: 1.8.472
  packs_version_avr8: 1.0.1443
  packs_version_qtouch: unknown
  packs_version_sam: 1.0.1726
  version_backend: 1.8.472
  version_frontend: ''
board:
  identifier: SAME54XplainedPro
  device: SAME54P20A-AU
details: null
application: null
middlewares: {}
drivers:
  CMCC:
    user_label: CMCC
    definition: Atmel:SAME54_Drivers:0.0.1::SAME54P20A-AU::CMCC::driver_config_definition::CMCC::HAL:HPL:CMCC
    functionality: System
    api: HAL:HPL:CMCC
    configuration:
      cache_size: 4 KB
      cmcc_advanced_configuration: false
      cmcc_clock_gating_disable: false
      cmcc_data_cache_disable: false
      cmcc_enable: false
      cmcc_inst_cache_disable: false
    optional_signals: []
    variant: null
    clocks:
      domain_group: null
  DMAC:
    user_label: DMAC
    definition: Atmel:SAME54_Drivers:0.0.1::SAME54P20A-AU::DMAC::driver_config_definition::DMAC::HAL:HPL:DMAC
    functionality: System
    api: HAL:HPL:DMAC
    configuration:
      dmac_beatsize_0: 8-bit bus transfer
      dmac_beatsize_1: 8-bit bus transfer
      dmac_beatsize_10: 8-bit bus transfer
      dmac_beatsize_11: 8-bit bus transfer
      dmac_beatsize_12: 8-bit bus transfer
      dmac_beatsize_13: 8-bit bus transfer
      dmac_beatsize_14: 8-bit bus transfer
      dmac_beatsize_15: 8-bit bus transfer
      dmac_beatsize_16: 8-bit bus transfer
      dmac_beatsize_17: 8-bit bus transfer
      dmac_beatsize_18: 8-bit bus transfer
      dmac_beatsize_19: 8-bit bus transfer
      dmac_beatsize_2: 8-bit bus transfer
      dmac_beatsize_20: 8-bit bus transfer
      dmac_beatsize_21: 8-bit bus transfer
      dmac_beatsize_22: 8-bit bus transfer
      dmac_beatsize_23: 8-bit bus transfer
      dmac_beatsize_24: 8-bit bus transfer
      dmac_beatsize_25: 8-bit bus transfer
      dmac_beatsize_26: 8-bit bus transfer
      dmac_beatsize_27: 8-bit bus transfer
      dmac_beatsize_28: 8-bit bus transfer
      dmac_beatsize_29: 8-bit bus transfer
      dmac_beatsize_3: 8-bit bus transfer
      dmac_beatsize_30: 8-bit bus transfer
      dmac_beatsize_31: 8-bit bus transfer
      dmac_beatsize_4: 8-bit bus transfer
      dmac_beatsize_5: 8-bit bus transfer
      dmac_beatsize_6: 8-bit bus transfer
      dmac_beatsize_7: 8-bit bus transfer
      dmac_beatsize_8: 8-bit bus transfer
      dmac_beatsize_9: 8-bit bus transfer
      dmac_blockact_0: Channel will be disabled if it is the last block transfer in
        the transaction
      dmac_blockact_1: Channel will be disabled if it is the last block transfer in
        the transaction
      dmac_blockact_10: Channel will be disabled if it is the last block transfer
        in the transaction
      dmac_blockact_11: Channel will be disabled if it is the last block transfer
        in the transaction
      dmac_blockact_12: Channel will be disabled if it is the last block transfer
        in the transaction
      dmac_blockact_13: Channel will be disabled if it is the last block transfer
        in the transaction
      dmac_blockact_14: Channel will be disabled if it is the last block transfer
        in the transaction
      dmac_blockact_15: Channel will be disabled if it is the last block transfer
        in the transaction
      dmac_blockact_16: Channel will be disabled if it is the last block transfer
        in the transaction
      dmac_blockact_17: Channel will be disabled if it is the last block transfer
        in the transaction
      dmac_blockact_18: Channel will be disabled if it is the last block transfer
        in the transaction
      dmac_blockact_19: Channel will be disabled if it is the last block transfer
        in the transaction
      dmac_blockact_2: Channel will be disabled if it is the last block transfer in
        the transaction
      dmac_blockact_20: Channel will be disabled if it is the last block transfer
        in the transaction
      dmac_blockact_21: Channel will be disabled if it is the last block transfer
        in the transaction
      dmac_blockact_22: Channel will be disabled if it is the last block transfer
        in the transaction
      dmac_blockact_23: Channel will be disabled if it is the last block transfer
        in the transaction
      dmac_blockact_24: Channel will be disabled if it is the last block transfer
        in the transaction
      dmac_blockact_25: Channel will be disabled if it is the last block transfer
        in the transaction
      dmac_blockact_26: Channel will be disabled if it is the last block transfer
        in the transaction
      dmac_blockact_27: Channel will be disabled if it is the last block transfer
        in the transaction
      dmac_blockact_28: Channel will be disabled if it is the last block transfer
        in the transaction
      dmac_blockact_29: Channel will be disabled if it is the last block transfer
        in the transaction
      dmac_blockact_3: Channel will be disabled if it is the last block transfer in
        the transaction
      dmac_blockact_30: Channel will be disabled if it is the last block transfer
        in the transaction
      dmac_blockact_31: Channel will be disabled if it is the last block transfer
        in the transaction
      dmac_blockact_4: Channel will be disabled if it is the last block transfer in
        the transaction
      dmac_blockact_5: Channel will be disabled if it is the last block transfer in
        the transaction
      dmac_blockact_6: Channel will be disabled if it is the last block transfer in
        the transaction
      dmac_blockact_7: Channel will be disabled if it is the last block transfer in
        the transaction
      dmac_blockact_8: Channel will be disabled if it is the last block transfer in
        the transaction
      dmac_blockact_9: Channel will be disabled if it is the last block transfer in
        the transaction
      dmac_channel_0_settings: false
      dmac_channel_10_settings: false
      dmac_channel_11_settings: false
      dmac_channel_12_settings: false
      dmac_channel_13_settings: false
      dmac_channel_14_settings: false
      dmac_channel_15_settings: false
      dmac_channel_16_settings: false
      dmac_channel_17_settings: false
      dmac_channel_18_settings: false
      dmac_channel_19_settings: false
      dmac_channel_1_settings: false
      dmac_channel_20_settings: false
      dmac_channel_21_settings: false
      dmac_channel_22_settings: false
      dmac_channel_23_settings: false
      dmac_channel_24_settings: false
      dmac_channel_25_settings: false
      dmac_channel_26_settings: false
      dmac_channel_27_settings: false
      dmac_channel_28_settings: false
      dmac_channel_29_settings: false
      dmac_channel_2_settings: false
      dmac_channel_30_settings: false
      dmac_channel_31_settings: false
      dmac_channel_3_settings: false
      dmac_channel_4_settings: false
      dmac_channel_5_settings: false
      dmac_channel_6_settings: false
      dmac_channel_7_settings: false
      dmac_channel_8_settings: false
      dmac_channel_9_settings: false
      dmac_dbgrun: false
      dmac_dstinc_0: false
      dmac_dstinc_1: false
      dmac_dstinc_10: false
      dmac_dstinc_11: false
      dmac_dstinc_12: false
      dmac_dstinc_13: false
      dmac_dstinc_14: false
      dmac_dstinc_15: false
      dmac_dstinc_16: false
      dmac_dstinc_17: false
      dmac_dstinc_18: false
      dmac_dstinc_19: false
      dmac_dstinc_2: false
      dmac_dstinc_20: false
      dmac_dstinc_21: false
      dmac_dstinc_22: false
      dmac_dstinc_23: false
      dmac_dstinc_24: false
      dmac_dstinc_25: false
      dmac_dstinc_26: false
      dmac_dstinc_27: false
      dmac_dstinc_28: false
      dmac_dstinc_29: false
      dmac_dstinc_3: false
      dmac_dstinc_30: false
      dmac_dstinc_31: false
      dmac_dstinc_4: false
      dmac_dstinc_5: false
      dmac_dstinc_6: false
      dmac_dstinc_7: false
      dmac_dstinc_8: false
      dmac_dstinc_9: false
      dmac_enable: false
      dmac_evact_0: No action
      dmac_evact_1: No action
      dmac_evact_10: No action
      dmac_evact_11: No action
      dmac_evact_12: No action
      dmac_evact_13: No action
      dmac_evact_14: No action
      dmac_evact_15: No action
      dmac_evact_16: No action
      dmac_evact_17: No action
      dmac_evact_18: No action
      dmac_evact_19: No action
      dmac_evact_2: No action
      dmac_evact_20: No action
      dmac_evact_21: No action
      dmac_evact_22: No action
      dmac_evact_23: No action
      dmac_evact_24: No action
      dmac_evact_25: No action
      dmac_evact_26: No action
      dmac_evact_27: No action
      dmac_evact_28: No action
      dmac_evact_29: No action
      dmac_evact_3: No action
      dmac_evact_30: No action
      dmac_evact_31: No action
      dmac_evact_4: No action
      dmac_evact_5: No action
      dmac_evact_6: No action
      dmac_evact_7: No action
      dmac_evact_8: No action
      dmac_evact_9: No action
      dmac_evie_0: false
      dmac_evie_1: false
      dmac_evie_10: false
      dmac_evie_11: false
      dmac_evie_12: false
      dmac_evie_13: false
      dmac_evie_14: false
      dmac_evie_15: false
      dmac_evie_16: false
      dmac_evie_17: false
      dmac_evie_18: false
      dmac_evie_19: false
      dmac_evie_2: false
      dmac_evie_20: false
      dmac_evie_21: false
      dmac_evie_22: false
      dmac_evie_23: false
      dmac_evie_24: false
      dmac_evie_25: false
      dmac_evie_26: false
      dmac_evie_27: false
      dmac_evie_28: false
      dmac_evie_29: false
      dmac_evie_3: false
      dmac_evie_30: false
      dmac_evie_31: false
      dmac_evie_4: false
      dmac_evie_5: false
      dmac_evie_6: false
      dmac_evie_7: false
      dmac_evie_8: false
      dmac_evie_9: false
      dmac_evoe_0: false
      dmac_evoe_1: false
      dmac_evoe_10: false
      dmac_evoe_11: false
      dmac_evoe_12: false
      dmac_evoe_13: false
      dmac_evoe_14: false
      dmac_evoe_15: false
      dmac_evoe_16: false
      dmac_evoe_17: false
      dmac_evoe_18: false
      dmac_evoe_19: false
      dmac_evoe_2: false
      dmac_evoe_20: false
      dmac_evoe_21: false
      dmac_evoe_22: false
      dmac_evoe_23: false
      dmac_evoe_24: false
      dmac_evoe_25: false
      dmac_evoe_26: false
      dmac_evoe_27: false
      dmac_evoe_28: false
      dmac_evoe_29: false
      dmac_evoe_3: false
      dmac_evoe_30: false
      dmac_evoe_31: false
      dmac_evoe_4: false
      dmac_evoe_5: false
      dmac_evoe_6: false
      dmac_evoe_7: false
      dmac_evoe_8: false
      dmac_evoe_9: false
      dmac_evosel_0: Event generation disabled
      dmac_evosel_1: Event generation disabled
      dmac_evosel_10: Event generation disabled
      dmac_evosel_11: Event generation disabled
      dmac_evosel_12: Event generation disabled
      dmac_evosel_13: Event generation disabled
      dmac_evosel_14: Event generation disabled
      dmac_evosel_15: Event generation disabled
      dmac_evosel_16: Event generation disabled
      dmac_evosel_17: Event generation disabled
      dmac_evosel_18: Event generation disabled
      dmac_evosel_19: Event generation disabled
      dmac_evosel_2: Event generation disabled
      dmac_evosel_20: Event generation disabled
      dmac_evosel_21: Event generation disabled
      dmac_evosel_22: Event generation disabled
      dmac_evosel_23: Event generation disabled
      dmac_evosel_24: Event generation disabled
      dmac_evosel_25: Event generation disabled
      dmac_evosel_26: Event generation disabled
      dmac_evosel_27: Event generation disabled
      dmac_evosel_28: Event generation disabled
      dmac_evosel_29: Event generation disabled
      dmac_evosel_3: Event generation disabled
      dmac_evosel_30: Event generation disabled
      dmac_evosel_31: Event generation disabled
      dmac_evosel_4: Event generation disabled
      dmac_evosel_5: Event generation disabled
      dmac_evosel_6: Event generation disabled
      dmac_evosel_7: Event generation disabled
      dmac_evosel_8: Event generation disabled
      dmac_evosel_9: Event generation disabled
      dmac_lvl_0: Channel priority 0
      dmac_lvl_1: Channel priority 0
      dmac_lvl_10: Channel priority 0
      dmac_lvl_11: Channel priority 0
      dmac_lvl_12: Channel priority 0
      dmac_lvl_13: Channel priority 0
      dmac_lvl_14: Channel priority 0
      dmac_lvl_15: Channel priority 0
      dmac_lvl_16: Channel priority 0
      dmac_lvl_17: Channel priority 0
      dmac_lvl_18: Channel priority 0
      dmac_lvl_19: Channel priority 0
      dmac_lvl_2: Channel priority 0
      dmac_lvl_20: Channel priority 0
      dmac_lvl_21: Channel priority 0
      dmac_lvl_22: Channel priority 0
      dmac_lvl_23: Channel priority 0
      dmac_lvl_24: Channel priority 0
      dmac_lvl_25: Channel priority 0
      dmac_lvl_26: Channel priority 0
      dmac_lvl_27: Channel priority 0
      dmac_lvl_28: Channel priority 0
      dmac_lvl_29: Channel priority 0
      dmac_lvl_3: Channel priority 0
      dmac_lvl_30: Channel priority 0
      dmac_lvl_31: Channel priority 0
      dmac_lvl_4: Channel priority 0
      dmac_lvl_5: Channel priority 0
      dmac_lvl_6: Channel priority 0
      dmac_lvl_7: Channel priority 0
      dmac_lvl_8: Channel priority 0
      dmac_lvl_9: Channel priority 0
      dmac_lvlen0: true
      dmac_lvlen1: true
      dmac_lvlen2: true
      dmac_lvlen3: true
      dmac_lvlpri0: 0
      dmac_lvlpri1: 0
      dmac_lvlpri2: 0
      dmac_lvlpri3: 0
      dmac_rrlvlen0: Static arbitration scheme for channel with priority 0
      dmac_rrlvlen1: Static arbitration scheme for channel with priority 1
      dmac_rrlvlen2: Static arbitration scheme for channel with priority 2
      dmac_rrlvlen3: Static arbitration scheme for channel with priority 3
      dmac_runstdby_0: false
      dmac_runstdby_1: false
      dmac_runstdby_10: false
      dmac_runstdby_11: false
      dmac_runstdby_12: false
      dmac_runstdby_13: false
      dmac_runstdby_14: false
      dmac_runstdby_15: false
      dmac_runstdby_16: false
      dmac_runstdby_17: false
      dmac_runstdby_18: false
      dmac_runstdby_19: false
      dmac_runstdby_2: false
      dmac_runstdby_20: false
      dmac_runstdby_21: false
      dmac_runstdby_22: false
      dmac_runstdby_23: false
      dmac_runstdby_24: false
      dmac_runstdby_25: false
      dmac_runstdby_26: false
      dmac_runstdby_27: false
      dmac_runstdby_28: false
      dmac_runstdby_29: false
      dmac_runstdby_3: false
      dmac_runstdby_30: false
      dmac_runstdby_31: false
      dmac_runstdby_4: false
      dmac_runstdby_5: false
      dmac_runstdby_6: false
      dmac_runstdby_7: false
      dmac_runstdby_8: false
      dmac_runstdby_9: false
      dmac_srcinc_0: false
      dmac_srcinc_1: false
      dmac_srcinc_10: false
      dmac_srcinc_11: false
      dmac_srcinc_12: false
      dmac_srcinc_13: false
      dmac_srcinc_14: false
      dmac_srcinc_15: false
      dmac_srcinc_16: false
      dmac_srcinc_17: false
      dmac_srcinc_18: false
      dmac_srcinc_19: false
      dmac_srcinc_2: false
      dmac_srcinc_20: false
      dmac_srcinc_21: false
      dmac_srcinc_22: false
      dmac_srcinc_23: false
      dmac_srcinc_24: false
      dmac_srcinc_25: false
      dmac_srcinc_26: false
      dmac_srcinc_27: false
      dmac_srcinc_28: false
      dmac_srcinc_29: false
      dmac_srcinc_3: false
      dmac_srcinc_30: false
      dmac_srcinc_31: false
      dmac_srcinc_4: false
      dmac_srcinc_5: false
      dmac_srcinc_6: false
      dmac_srcinc_7: false
      dmac_srcinc_8: false
      dmac_srcinc_9: false
      dmac_stepsel_0: Step size settings apply to the destination address
      dmac_stepsel_1: Step size settings apply to the destination address
      dmac_stepsel_10: Step size settings apply to the destination address
      dmac_stepsel_11: Step size settings apply to the destination address
      dmac_stepsel_12: Step size settings apply to the destination address
      dmac_stepsel_13: Step size settings apply to the destination address
      dmac_stepsel_14: Step size settings apply to the destination address
      dmac_stepsel_15: Step size settings apply to the destination address
      dmac_stepsel_16: Step size settings apply to the destination address
      dmac_stepsel_17: Step size settings apply to the destination address
      dmac_stepsel_18: Step size settings apply to the destination address
      dmac_stepsel_19: Step size settings apply to the destination address
      dmac_stepsel_2: Step size settings apply to the destination address
      dmac_stepsel_20: Step size settings apply to the destination address
      dmac_stepsel_21: Step size settings apply to the destination address
      dmac_stepsel_22: Step size settings apply to the destination address
      dmac_stepsel_23: Step size settings apply to the destination address
      dmac_stepsel_24: Step size settings apply to the destination address
      dmac_stepsel_25: Step size settings apply to the destination address
      dmac_stepsel_26: Step size settings apply to the destination address
      dmac_stepsel_27: Step size settings apply to the destination address
      dmac_stepsel_28: Step size settings apply to the destination address
      dmac_stepsel_29: Step size settings apply to the destination address
      dmac_stepsel_3: Step size settings apply to the destination address
      dmac_stepsel_30: Step size settings apply to the destination address
      dmac_stepsel_31: Step size settings apply to the destination address
      dmac_stepsel_4: Step size settings apply to the destination address
      dmac_stepsel_5: Step size settings apply to the destination address
      dmac_stepsel_6: Step size settings apply to the destination address
      dmac_stepsel_7: Step size settings apply to the destination address
      dmac_stepsel_8: Step size settings apply to the destination address
      dmac_stepsel_9: Step size settings apply to the destination address
      dmac_stepsize_0: Next ADDR = ADDR + (BEATSIZE + 1) * 1
      dmac_stepsize_1: Next ADDR = ADDR + (BEATSIZE + 1) * 1
      dmac_stepsize_10: Next ADDR = ADDR + (BEATSIZE + 1) * 1
      dmac_stepsize_11: Next ADDR = ADDR + (BEATSIZE + 1) * 1
      dmac_stepsize_12: Next ADDR = ADDR + (BEATSIZE + 1) * 1
      dmac_stepsize_13: Next ADDR = ADDR + (BEATSIZE + 1) * 1
      dmac_stepsize_14: Next ADDR = ADDR + (BEATSIZE + 1) * 1
      dmac_stepsize_15: Next ADDR = ADDR + (BEATSIZE + 1) * 1
      dmac_stepsize_16: Next ADDR = ADDR + (BEATSIZE + 1) * 1
      dmac_stepsize_17: Next ADDR = ADDR + (BEATSIZE + 1) * 1
      dmac_stepsize_18: Next ADDR = ADDR + (BEATSIZE + 1) * 1
      dmac_stepsize_19: Next ADDR = ADDR + (BEATSIZE + 1) * 1
      dmac_stepsize_2: Next ADDR = ADDR + (BEATSIZE + 1) * 1
      dmac_stepsize_20: Next ADDR = ADDR + (BEATSIZE + 1) * 1
      dmac_stepsize_21: Next ADDR = ADDR + (BEATSIZE + 1) * 1
      dmac_stepsize_22: Next ADDR = ADDR + (BEATSIZE + 1) * 1
      dmac_stepsize_23: Next ADDR = ADDR + (BEATSIZE + 1) * 1
      dmac_stepsize_24: Next ADDR = ADDR + (BEATSIZE + 1) * 1
      dmac_stepsize_25: Next ADDR = ADDR + (BEATSIZE + 1) * 1
      dmac_stepsize_26: Next ADDR = ADDR + (BEATSIZE + 1) * 1
      dmac_stepsize_27: Next ADDR = ADDR + (BEATSIZE + 1) * 1
      dmac_stepsize_28: Next ADDR = ADDR + (BEATSIZE + 1) * 1
      dmac_stepsize_29: Next ADDR = ADDR + (BEATSIZE + 1) * 1
      dmac_stepsize_3: Next ADDR = ADDR + (BEATSIZE + 1) * 1
      dmac_stepsize_30: Next ADDR = ADDR + (BEATSIZE + 1) * 1
      dmac_stepsize_31: Next ADDR = ADDR + (BEATSIZE + 1) * 1
      dmac_stepsize_4: Next ADDR = ADDR + (BEATSIZE + 1) * 1
      dmac_stepsize_5: Next ADDR = ADDR + (BEATSIZE + 1) * 1
      dmac_stepsize_6: Next ADDR = ADDR + (BEATSIZE + 1) * 1
      dmac_stepsize_7: Next ADDR = ADDR + (BEATSIZE + 1) * 1
      dmac_stepsize_8: Next ADDR = ADDR + (BEATSIZE + 1) * 1
      dmac_stepsize_9: Next ADDR = ADDR + (BEATSIZE + 1) * 1
      dmac_trifsrc_0: Only software/event triggers
      dmac_trifsrc_1: Only software/event triggers
      dmac_trifsrc_10: Only software/event triggers
      dmac_trifsrc_11: Only software/event triggers
      dmac_trifsrc_12: Only software/event triggers
      dmac_trifsrc_13: Only software/event triggers
      dmac_trifsrc_14: Only software/event triggers
      dmac_trifsrc_15: Only software/event triggers
      dmac_trifsrc_16: Only software/event triggers
      dmac_trifsrc_17: Only software/event triggers
      dmac_trifsrc_18: Only software/event triggers
      dmac_trifsrc_19: Only software/event triggers
      dmac_trifsrc_2: Only software/event triggers
      dmac_trifsrc_20: Only software/event triggers
      dmac_trifsrc_21: Only software/event triggers
      dmac_trifsrc_22: Only software/event triggers
      dmac_trifsrc_23: Only software/event triggers
      dmac_trifsrc_24: Only software/event triggers
      dmac_trifsrc_25: Only software/event triggers
      dmac_trifsrc_26: Only software/event triggers
      dmac_trifsrc_27: Only software/event triggers
      dmac_trifsrc_28: Only software/event triggers
      dmac_trifsrc_29: Only software/event triggers
      dmac_trifsrc_3: Only software/event triggers
      dmac_trifsrc_30: Only software/event triggers
      dmac_trifsrc_31: Only software/event triggers
      dmac_trifsrc_4: Only software/event triggers
      dmac_trifsrc_5: Only software/event triggers
      dmac_trifsrc_6: Only software/event triggers
      dmac_trifsrc_7: Only software/event triggers
      dmac_trifsrc_8: Only software/event triggers
      dmac_trifsrc_9: Only software/event triggers
      dmac_trigact_0: One trigger required for each block transfer
      dmac_trigact_1: One trigger required for each block transfer
      dmac_trigact_10: One trigger required for each block transfer
      dmac_trigact_11: One trigger required for each block transfer
      dmac_trigact_12: One trigger required for each block transfer
      dmac_trigact_13: One trigger required for each block transfer
      dmac_trigact_14: One trigger required for each block transfer
      dmac_trigact_15: One trigger required for each block transfer
      dmac_trigact_16: One trigger required for each block transfer
      dmac_trigact_17: One trigger required for each block transfer
      dmac_trigact_18: One trigger required for each block transfer
      dmac_trigact_19: One trigger required for each block transfer
      dmac_trigact_2: One trigger required for each block transfer
      dmac_trigact_20: One trigger required for each block transfer
      dmac_trigact_21: One trigger required for each block transfer
      dmac_trigact_22: One trigger required for each block transfer
      dmac_trigact_23: One trigger required for each block transfer
      dmac_trigact_24: One trigger required for each block transfer
      dmac_trigact_25: One trigger required for each block transfer
      dmac_trigact_26: One trigger required for each block transfer
      dmac_trigact_27: One trigger required for each block transfer
      dmac_trigact_28: One trigger required for each block transfer
      dmac_trigact_29: One trigger required for each block transfer
      dmac_trigact_3: One trigger required for each block transfer
      dmac_trigact_30: One trigger required for each block transfer
      dmac_trigact_31: One trigger required for each block transfer
      dmac_trigact_4: One trigger required for each block transfer
      dmac_trigact_5: One trigger required for each block transfer
      dmac_trigact_6: One trigger required for each block transfer
      dmac_trigact_7: One trigger required for each block transfer
      dmac_trigact_8: One trigger required for each block transfer
      dmac_trigact_9: One trigger required for each block transfer
    optional_signals: []
    variant: null
    clocks:
      domain_group: null
  GCLK:
    user_label: GCLK
    definition: Atmel:SAME54_Drivers:0.0.1::SAME54P20A-AU::GCLK::driver_config_definition::GCLK::HAL:HPL:GCLK
    functionality: System
    api: HAL:HPL:GCLK
    configuration:
      $input: 12000000
      $input_id: External Crystal Oscillator 8-48MHz (XOSC1)
      RESERVED_InputFreq: 12000000
      RESERVED_InputFreq_id: External Crystal Oscillator 8-48MHz (XOSC1)
      _$freq_output_Generic clock generator 0: 48005120
      _$freq_output_Generic clock generator 1: 48005120
      _$freq_output_Generic clock generator 10: 12000000
      _$freq_output_Generic clock generator 11: 12000000
      _$freq_output_Generic clock generator 2: 3000000
      _$freq_output_Generic clock generator 3: 32768
      _$freq_output_Generic clock generator 4: 12000000
      _$freq_output_Generic clock generator 5: 12000000
      _$freq_output_Generic clock generator 6: 12000000
      _$freq_output_Generic clock generator 7: 12000000
      _$freq_output_Generic clock generator 8: 12000000
      _$freq_output_Generic clock generator 9: 12000000
      enable_gclk_gen_0: true
      enable_gclk_gen_0__externalclock: 1000000
      enable_gclk_gen_1: false
      enable_gclk_gen_10: false
      enable_gclk_gen_10__externalclock: 1000000
      enable_gclk_gen_11: false
      enable_gclk_gen_11__externalclock: 1000000
      enable_gclk_gen_1__externalclock: 1000000
      enable_gclk_gen_2: false
      enable_gclk_gen_2__externalclock: 1000000
      enable_gclk_gen_3: true
      enable_gclk_gen_3__externalclock: 1000000
      enable_gclk_gen_4: false
      enable_gclk_gen_4__externalclock: 1000000
      enable_gclk_gen_5: false
      enable_gclk_gen_5__externalclock: 1000000
      enable_gclk_gen_6: false
      enable_gclk_gen_6__externalclock: 1000000
      enable_gclk_gen_7: false
      enable_gclk_gen_7__externalclock: 1000000
      enable_gclk_gen_8: false
      enable_gclk_gen_8__externalclock: 1000000
      enable_gclk_gen_9: false
      enable_gclk_gen_9__externalclock: 1000000
      gclk_arch_gen_0_enable: true
      gclk_arch_gen_0_idc: false
      gclk_arch_gen_0_oe: false
      gclk_arch_gen_0_oov: false
      gclk_arch_gen_0_runstdby: false
      gclk_arch_gen_10_enable: false
      gclk_arch_gen_10_idc: false
      gclk_arch_gen_10_oe: false
      gclk_arch_gen_10_oov: false
      gclk_arch_gen_10_runstdby: false
      gclk_arch_gen_11_enable: false
      gclk_arch_gen_11_idc: false
      gclk_arch_gen_11_oe: false
      gclk_arch_gen_11_oov: false
      gclk_arch_gen_11_runstdby: false
      gclk_arch_gen_1_enable: false
      gclk_arch_gen_1_idc: false
      gclk_arch_gen_1_oe: false
      gclk_arch_gen_1_oov: false
      gclk_arch_gen_1_runstdby: false
      gclk_arch_gen_2_enable: false
      gclk_arch_gen_2_idc: false
      gclk_arch_gen_2_oe: false
      gclk_arch_gen_2_oov: false
      gclk_arch_gen_2_runstdby: false
      gclk_arch_gen_3_enable: true
      gclk_arch_gen_3_idc: false
      gclk_arch_gen_3_oe: false
      gclk_arch_gen_3_oov: false
      gclk_arch_gen_3_runstdby: false
      gclk_arch_gen_4_enable: false
      gclk_arch_gen_4_idc: false
      gclk_arch_gen_4_oe: false
      gclk_arch_gen_4_oov: false
      gclk_arch_gen_4_runstdby: false
      gclk_arch_gen_5_enable: false
      gclk_arch_gen_5_idc: false
      gclk_arch_gen_5_oe: false
      gclk_arch_gen_5_oov: false
      gclk_arch_gen_5_runstdby: false
      gclk_arch_gen_6_enable: false
      gclk_arch_gen_6_idc: false
      gclk_arch_gen_6_oe: false
      gclk_arch_gen_6_oov: false
      gclk_arch_gen_6_runstdby: false
      gclk_arch_gen_7_enable: false
      gclk_arch_gen_7_idc: false
      gclk_arch_gen_7_oe: false
      gclk_arch_gen_7_oov: false
      gclk_arch_gen_7_runstdby: false
      gclk_arch_gen_8_enable: false
      gclk_arch_gen_8_idc: false
      gclk_arch_gen_8_oe: false
      gclk_arch_gen_8_oov: false
      gclk_arch_gen_8_runstdby: false
      gclk_arch_gen_9_enable: false
      gclk_arch_gen_9_idc: false
      gclk_arch_gen_9_oe: false
      gclk_arch_gen_9_oov: false
      gclk_arch_gen_9_runstdby: false
      gclk_gen_0_div: 1
      gclk_gen_0_div_sel: false
      gclk_gen_0_oscillator: Digital Frequency Locked Loop (DFLL48M)
      gclk_gen_10_div: 1
      gclk_gen_10_div_sel: false
      gclk_gen_10_oscillator: External Crystal Oscillator 8-48MHz (XOSC1)
      gclk_gen_11_div: 1
      gclk_gen_11_div_sel: false
      gclk_gen_11_oscillator: External Crystal Oscillator 8-48MHz (XOSC1)
      gclk_gen_1_div: 1
      gclk_gen_1_div_sel: false
      gclk_gen_1_oscillator: Digital Frequency Locked Loop (DFLL48M)
      gclk_gen_2_div: 1
      gclk_gen_2_div_sel: true
      gclk_gen_2_oscillator: External Crystal Oscillator 8-48MHz (XOSC1)
      gclk_gen_3_div: 1
      gclk_gen_3_div_sel: false
      gclk_gen_3_oscillator: 32kHz External Crystal Oscillator (XOSC32K)
      gclk_gen_4_div: 1
      gclk_gen_4_div_sel: false
      gclk_gen_4_oscillator: External Crystal Oscillator 8-48MHz (XOSC1)
      gclk_gen_5_div: 1
      gclk_gen_5_div_sel: false
      gclk_gen_5_oscillator: External Crystal Oscillator 8-48MHz (XOSC1)
      gclk_gen_6_div: 1
      gclk_gen_6_div_sel: false
      gclk_gen_6_oscillator: External Crystal Oscillator 8-48MHz (XOSC1)
      gclk_gen_7_div: 1
      gclk_gen_7_div_sel: false
      gclk_gen_7_oscillator: External Crystal Oscillator 8-48MHz (XOSC1)
      gclk_gen_8_div: 1
      gclk_gen_8_div_sel: false
      gclk_gen_8_oscillator: External Crystal Oscillator 8-48MHz (XOSC1)
      gclk_gen_9_div: 1
      gclk_gen_9_div_sel: false
      gclk_gen_9_oscillator: External Crystal Oscillator 8-48MHz (XOSC1)
    optional_signals: []
    variant: null
    clocks:
      domain_group: null
  MCLK:
    user_label: MCLK
    definition: Atmel:SAME54_Drivers:0.0.1::SAME54P20A-AU::MCLK::driver_config_definition::MCLK::HAL:HPL:MCLK
    functionality: System
    api: HAL:HPL:MCLK
    configuration:
      $input: 48005120
      $input_id: Generic clock generator 0
      RESERVED_InputFreq: 48005120
      RESERVED_InputFreq_id: Generic clock generator 0
      _$freq_output_CPU: 48005120
      cpu_clock_source: Generic clock generator 0
      cpu_div: '1'
      enable_cpu_clock: true
      mclk_arch_bupdiv: Divide by 8
      mclk_arch_hsdiv: Divide by 1
      mclk_arch_lpdiv: Divide by 4
      nvm_wait_states: '0'
    optional_signals: []
    variant: null
    clocks:
      domain_group:
        nodes:
        - name: CPU
          input: CPU
          external: false
          external_frequency: 0
        configuration: {}
  OSC32KCTRL:
    user_label: OSC32KCTRL
    definition: Atmel:SAME54_Drivers:0.0.1::SAME54P20A-AU::OSC32KCTRL::driver_config_definition::OSC32KCTRL::HAL:HPL:OSC32KCTRL
    functionality: System
    api: HAL:HPL:OSC32KCTRL
    configuration:
      $input: 32768
      $input_id: 32kHz Ultra Low Power Internal Oscillator (OSCULP32K)
      RESERVED_InputFreq: 32768
      RESERVED_InputFreq_id: 32kHz Ultra Low Power Internal Oscillator (OSCULP32K)
      _$freq_output_RTC source: 32768
      enable_osculp32k: true
      enable_rtc_source: false
      enable_xosc32k: true
      osculp32k_calib: 0
      osculp32k_calib_enable: false
      rtc_1khz_selection: false
      rtc_source_oscillator: 32kHz Ultra Low Power Internal Oscillator (OSCULP32K)
      xosc32k_arch_cfden: false
      xosc32k_arch_cfdeo: false
      xosc32k_arch_cgm: Standard mode
      xosc32k_arch_en1k: false
      xosc32k_arch_en32k: false
      xosc32k_arch_enable: true
      xosc32k_arch_ondemand: true
      xosc32k_arch_runstdby: false
      xosc32k_arch_startup: 62592us
      xosc32k_arch_swben: false
      xosc32k_arch_xtalen: true
    optional_signals: []
    variant: null
    clocks:
      domain_group: null
  OSCCTRL:
    user_label: OSCCTRL
    definition: Atmel:SAME54_Drivers:0.0.1::SAME54P20A-AU::OSCCTRL::driver_config_definition::OSCCTRL::HAL:HPL:OSCCTRL
    functionality: System
    api: HAL:HPL:OSCCTRL
    configuration:
      $input: 32768
      $input_id: 32kHz External Crystal Oscillator (XOSC32K)
      RESERVED_InputFreq: 32768
      RESERVED_InputFreq_id: 32kHz External Crystal Oscillator (XOSC32K)
      _$freq_output_Digital Frequency Locked Loop (DFLL48M): 48005120
      _$freq_output_Digital Phase Locked Loop (DPLL0): 47985664
      _$freq_output_Digital Phase Locked Loop (DPLL1): 47985664
      _$freq_output_External Crystal Oscillator 8-48MHz (XOSC0): '12000000'
      _$freq_output_External Crystal Oscillator 8-48MHz (XOSC1): '12000000'
      dfll_arch_bplckc: false
      dfll_arch_calibration: false
      dfll_arch_ccdis: true
      dfll_arch_coarse: 31
      dfll_arch_cstep: 1
      dfll_arch_enable: true
      dfll_arch_fine: 128
      dfll_arch_fstep: 1
      dfll_arch_llaw: false
      dfll_arch_ondemand: false
      dfll_arch_qldis: false
      dfll_arch_runstdby: false
      dfll_arch_stable: false
      dfll_arch_usbcrm: false
      dfll_arch_waitlock: false
      dfll_mode: Closed Loop Mode
      dfll_mul: 1465
      dfll_ref_clock: Generic clock generator 3
      enable_dfll: true
      enable_fdpll0: false
      enable_fdpll1: false
      enable_xosc0: false
      enable_xosc1: false
      fdpll0_arch_dcoen: false
      fdpll0_arch_enable: false
      fdpll0_arch_filter: 0
      fdpll0_arch_lbypass: false
      fdpll0_arch_ltime: No time-out, automatic lock
      fdpll0_arch_ondemand: false
      fdpll0_arch_refclk: XOSC32K clock reference
      fdpll0_arch_runstdby: false
      fdpll0_arch_wuf: false
      fdpll0_clock_dcofilter: 0
      fdpll0_clock_div: 0
      fdpll0_ldr: 1463
      fdpll0_ldrfrac: 13
      fdpll0_ref_clock: 32kHz External Crystal Oscillator (XOSC32K)
      fdpll1_arch_dcoen: false
      fdpll1_arch_enable: false
      fdpll1_arch_filter: 0
      fdpll1_arch_lbypass: false
      fdpll1_arch_ltime: No time-out, automatic lock
      fdpll1_arch_ondemand: false
      fdpll1_arch_refclk: XOSC32K clock reference
      fdpll1_arch_runstdby: false
      fdpll1_arch_wuf: false
      fdpll1_clock_dcofilter: 0
      fdpll1_clock_div: 0
      fdpll1_ldr: 1463
      fdpll1_ldrfrac: 13
      fdpll1_ref_clock: 32kHz External Crystal Oscillator (XOSC32K)
      xosc0_arch_cfden: false
      xosc0_arch_enable: false
      xosc0_arch_enalc: false
      xosc0_arch_lowbufgain: false
      xosc0_arch_ondemand: false
      xosc0_arch_runstdby: false
      xosc0_arch_startup: 31us
      xosc0_arch_swben: false
      xosc0_arch_xtalen: false
      xosc0_frequency: 12000000
      xosc1_arch_cfden: false
      xosc1_arch_enable: false
      xosc1_arch_enalc: false
      xosc1_arch_lowbufgain: false
      xosc1_arch_ondemand: false
      xosc1_arch_runstdby: false
      xosc1_arch_startup: 31us
      xosc1_arch_swben: false
      xosc1_arch_xtalen: true
      xosc1_frequency: 12000000
    optional_signals: []
    variant: null
    clocks:
      domain_group: null
  PORT:
    user_label: PORT
    definition: Atmel:SAME54_Drivers:0.0.1::SAME54P20A-AU::PORT::driver_config_definition::PORT::HAL:HPL:PORT
    functionality: System
    api: HAL:HPL:PORT
    configuration:
      enable_port_input_event_0: false
      enable_port_input_event_1: false
      enable_port_input_event_2: false
      enable_port_input_event_3: false
      porta_event_action_0: Output register of pin will be set to level of event
      porta_event_action_1: Output register of pin will be set to level of event
      porta_event_action_2: Output register of pin will be set to level of event
      porta_event_action_3: Output register of pin will be set to level of event
      porta_event_pin_identifier_0: 0
      porta_event_pin_identifier_1: 0
      porta_event_pin_identifier_2: 0
      porta_event_pin_identifier_3: 0
      porta_input_event_enable_0: false
      porta_input_event_enable_1: false
      porta_input_event_enable_2: false
      porta_input_event_enable_3: false
      portb_event_action_0: Output register of pin will be set to level of event
      portb_event_action_1: Output register of pin will be set to level of event
      portb_event_action_2: Output register of pin will be set to level of event
      portb_event_action_3: Output register of pin will be set to level of event
      portb_event_pin_identifier_0: 0
      portb_event_pin_identifier_1: 0
      portb_event_pin_identifier_2: 0
      portb_event_pin_identifier_3: 0
      portb_input_event_enable_0: false
      portb_input_event_enable_1: false
      portb_input_event_enable_2: false
      portb_input_event_enable_3: false
      portc_event_action_0: Output register of pin will be set to level of event
      portc_event_action_1: Output register of pin will be set to level of event
      portc_event_action_2: Output register of pin will be set to level of event
      portc_event_action_3: Output register of pin will be set to level of event
      portc_event_pin_identifier_0: 0
      portc_event_pin_identifier_1: 0
      portc_event_pin_identifier_2: 0
      portc_event_pin_identifier_3: 0
      portc_input_event_enable_0: false
      portc_input_event_enable_1: false
      portc_input_event_enable_2: false
      portc_input_event_enable_3: false
      portd_event_action_0: Output register of pin will be set to level of event
      portd_event_action_1: Output register of pin will be set to level of event
      portd_event_action_2: Output register of pin will be set to level of event
      portd_event_action_3: Output register of pin will be set to level of event
      portd_event_pin_identifier_0: 0
      portd_event_pin_identifier_1: 0
      portd_event_pin_identifier_2: 0
      portd_event_pin_identifier_3: 0
      portd_input_event_enable_0: false
      portd_input_event_enable_1: false
      portd_input_event_enable_2: false
      portd_input_event_enable_3: false
    optional_signals: []
    variant: null
    clocks:
      domain_group: null
  RAMECC:
    user_label: RAMECC
    definition: Atmel:SAME54_Drivers:0.0.1::SAME54P20A-AU::RAMECC::driver_config_definition::RAMECC::HAL:HPL:RAMECC
    functionality: System
    api: HAL:HPL:RAMECC
    configuration: {}
    optional_signals: []
    variant: null
    clocks:
      domain_group: null
  USART_DBG:
    user_label: USART_DBG
    definition: Atmel:SAME54_Drivers:0.0.1::SAME54P20A-AU::SERCOM2::driver_config_definition::UART::HAL:Driver:USART.Sync
    functionality: USART
    api: HAL:Driver:USART_Sync
    configuration:
      usart_advanced: false
      usart_arch_clock_mode: USART with internal clock
      usart_arch_cloden: false
      usart_arch_dbgstop: Keep running
      usart_arch_dord: LSB is transmitted first
      usart_arch_enc: No encoding
      usart_arch_fractional: 0
      usart_arch_ibon: false
      usart_arch_lin_slave_enable: Disable
      usart_arch_runstdby: false
      usart_arch_sampa: 7-8-9 (3-4-5 8-bit over-sampling)
      usart_arch_sampr: 16x arithmetic
      usart_arch_sfde: false
      usart_baud_rate: 115200
      usart_character_size: 8 bits
      usart_parity: No parity
      usart_rx_enable: true
      usart_stop_bit: One stop bit
      usart_tx_enable: true
    optional_signals: []
    variant:
      specification: TXPO=0, RXPO=1, CMODE=0
      required_signals:
      - name: SERCOM2/PAD/0
        pad: PB25
        label: TX
      - name: SERCOM2/PAD/1
        pad: PB24
        label: RX
    clocks:
      domain_group:
        nodes:
        - name: Core
          input: Generic clock generator 0
          external: false
          external_frequency: 0
        - name: Slow
          input: Generic clock generator 3
          external: false
          external_frequency: 0
        configuration:
          core_gclk_selection: Generic clock generator 0
          slow_gclk_selection: Generic clock generator 3
  SPI_SD_MMC:
    user_label: SPI_SD_MMC
    definition: Atmel:SAME54_Drivers:0.0.1::SAME54P20A-AU::SERCOM4::driver_config_definition::SPI.Master::HAL:Driver:SPI.Master.Sync
    functionality: SPI
    api: HAL:Driver:SPI_Master_Sync
    configuration:
      spi_master_advanced: false
      spi_master_arch_cpha: Sample input on leading edge
      spi_master_arch_cpol: SCK is low when idle
      spi_master_arch_dbgstop: Keep running
      spi_master_arch_dord: MSB first
      spi_master_arch_ibon: In data stream
      spi_master_arch_runstdby: false
      spi_master_baud_rate: 50000
      spi_master_character_size: 8 bits
      spi_master_dummybyte: 511
      spi_master_rx_enable: true
    optional_signals: []
    variant:
      specification: TXPO=0, RXPO=3
      required_signals:
      - name: SERCOM4/PAD/0
        pad: PB27
        label: MOSI
      - name: SERCOM4/PAD/1
        pad: PB26
        label: SCK
      - name: SERCOM4/PAD/3
        pad: PB29
        label: MISO
    clocks:
      domain_group:
        nodes:
        - name: Core
          input: Generic clock generator 0
          external: false
          external_frequency: 0
        - name: Slow
          input: Generic clock generator 3
          external: false
          external_frequency: 0
        configuration:
          core_gclk_selection: Generic clock generator 0
          slow_gclk_selection: Generic clock generator 3
  DELAY_0:
    user_label: DELAY_0
    definition: Atmel:SAME54_Drivers:0.0.1::SAME54P20A-AU::SysTick::driver_config_definition::Delay::HAL:Driver:Delay
    functionality: Delay
    api: HAL:Driver:Delay
    configuration:
      systick_arch_tickint: false
    optional_signals: []
    variant: null
    clocks:
      domain_group: null
pads:
  PB24:
    name: PB24
    definition: Atmel:SAME54_Drivers:0.0.1::SAME54P20A-AU::pad::PB24
    mode: Peripheral IO
    user_label: PB24
    configuration: null
  PB25:
    name: PB25
    definition: Atmel:SAME54_Drivers:0.0.1::SAME54P20A-AU::pad::PB25
    mode: Peripheral IO
    user_label: PB25
    configuration: null
  PB26:
    name: PB26
    definition: Atmel:SAME54_Drivers:0.0.1::SAME54P20A-AU::pad::PB26
    mode: Digital output
    user_label: PB26
    configuration: null
  PB27:
    name: PB27
    definition: Atmel:SAME54_Drivers:0.0.1::SAME54P20A-AU::pad::PB27
    mode: Digital output
    user_label: PB27
    configuration: null
  PB29:
    name: PB29
    definition: Atmel:SAME54_Drivers:0.0.1::SAME54P20A-AU::pad::PB29
    mode: Digital input
    user_label: PB29
    configuration: null
toolchain_options: []
