EESchema Schematic File Version 4
EELAYER 30 0
EELAYER END
$Descr A4 11693 8268
encoding utf-8
Sheet 2 5
Title "Aquatic Robotic Courier - Boat 0"
Date "2020-10-01"
Rev "1"
Comp "ePenguin"
Comment1 "Author: Penguin"
Comment2 ""
Comment3 ""
Comment4 ""
$EndDescr
$Comp
L MCU_Microchip_SAMD:ATSAMD21E18A-A U?
U 1 1 5F782E9E
P 1850 3800
AR Path="/5F782E9E" Ref="U?"  Part="1" 
AR Path="/5F7734A5/5F782E9E" Ref="U1"  Part="1" 
F 0 "U1" H 2480 3846 50  0000 L CNN
F 1 "ATSAMD21E18A-A" H 2480 3755 50  0000 L CNN
F 2 "Package_QFP:TQFP-32_7x7mm_P0.8mm" H 2750 1950 50  0001 C CNN
F 3 "http://ww1.microchip.com/downloads/en/DeviceDoc/SAM_D21_DA1_Family_Data%20Sheet_DS40001882E.pdf" H 1850 3800 50  0001 C CNN
	1    1850 3800
	1    0    0    -1  
$EndComp
$Comp
L power:GND #PWR0101
U 1 1 5F78448A
P 4350 2900
F 0 "#PWR0101" H 4350 2650 50  0001 C CNN
F 1 "GND" H 4355 2727 50  0000 C CNN
F 2 "" H 4350 2900 50  0001 C CNN
F 3 "" H 4350 2900 50  0001 C CNN
	1    4350 2900
	1    0    0    -1  
$EndComp
Wire Wire Line
	4350 2800 4400 2800
Connection ~ 4350 2800
Wire Wire Line
	4350 2800 4350 2900
Wire Wire Line
	4400 2800 4400 2700
Wire Wire Line
	4300 2800 4350 2800
Wire Wire Line
	4300 2700 4300 2800
$Comp
L power:+3V3 #PWR0102
U 1 1 5F784496
P 4400 1300
F 0 "#PWR0102" H 4400 1150 50  0001 C CNN
F 1 "+3V3" H 4415 1473 50  0000 C CNN
F 2 "" H 4400 1300 50  0001 C CNN
F 3 "" H 4400 1300 50  0001 C CNN
	1    4400 1300
	1    0    0    -1  
$EndComp
Wire Wire Line
	4400 1500 4400 1300
$Comp
L Connector:Conn_ARM_JTAG_SWD_10 J1
U 1 1 5F78449D
P 4400 2100
F 0 "J1" H 3957 2146 50  0000 R CNN
F 1 "ARM_SWD_10_Pin" H 3957 2055 50  0000 R CNN
F 2 "Connector_PinHeader_1.27mm:PinHeader_2x05_P1.27mm_Horizontal" H 4400 2100 50  0001 C CNN
F 3 "http://infocenter.arm.com/help/topic/com.arm.doc.ddi0314h/DDI0314H_coresight_components_trm.pdf" V 4050 850 50  0001 C CNN
	1    4400 2100
	1    0    0    -1  
$EndComp
Text HLabel 800  650  0    50   Input ~ 0
Vcc
Wire Wire Line
	800  650  1300 650 
Text Label 1300 650  0    50   ~ 0
VCC
Text HLabel 850  800  0    50   Input ~ 0
USBDP
Text HLabel 850  950  0    50   Input ~ 0
USBDM
Wire Wire Line
	850  800  1300 800 
Text Label 1300 800  0    50   ~ 0
USBDP
Wire Wire Line
	850  950  1300 950 
Text Label 1300 950  0    50   ~ 0
USBDM
$EndSCHEMATC
