EESchema Schematic File Version 4
EELAYER 30 0
EELAYER END
$Descr A4 11693 8268
encoding utf-8
Sheet 1 1
Title ""
Date ""
Rev ""
Comp ""
Comment1 ""
Comment2 ""
Comment3 ""
Comment4 ""
$EndDescr
$Comp
L plib:Conn_ARM_SWD_10_DEBUG J1
U 1 1 5FC75444
P 3775 3175
F 0 "J1" H 3331 2821 50  0000 R CNN
F 1 "Conn_ARM_SWD_10_DEBUG" H 3331 2730 50  0000 R CNN
F 2 "plib:DebugEdge_2x05" H 3775 3175 50  0001 C CNN
F 3 "http://infocenter.arm.com/help/topic/com.arm.doc.ddi0314h/DDI0314H_coresight_components_trm.pdf" V 3425 1925 50  0001 C CNN
	1    3775 3175
	1    0    0    -1  
$EndComp
Wire Wire Line
	4275 2875 5425 2875
Wire Wire Line
	4275 3075 5425 3075
Wire Wire Line
	4275 3175 5425 3175
Wire Wire Line
	4275 3275 5425 3275
Wire Wire Line
	5925 3775 5925 3875
Wire Wire Line
	5925 3875 5975 3875
Wire Wire Line
	6025 3875 6025 3775
Wire Wire Line
	5975 3875 5975 4000
Connection ~ 5975 3875
Wire Wire Line
	5975 3875 6025 3875
$Comp
L power:GND #PWR03
U 1 1 5FC7A36D
P 5975 4000
F 0 "#PWR03" H 5975 3750 50  0001 C CNN
F 1 "GND" H 5980 3827 50  0000 C CNN
F 2 "" H 5975 4000 50  0001 C CNN
F 3 "" H 5975 4000 50  0001 C CNN
	1    5975 4000
	1    0    0    -1  
$EndComp
Wire Wire Line
	3775 2575 3775 2450
Wire Wire Line
	3775 2450 5925 2450
Wire Wire Line
	5925 2450 5925 2575
Wire Wire Line
	3525 4575 3525 4650
Wire Wire Line
	3525 4650 3625 4650
Wire Wire Line
	3625 4650 3625 4575
Wire Wire Line
	3625 4650 3725 4650
Wire Wire Line
	3725 4650 3725 4575
Connection ~ 3625 4650
Wire Wire Line
	3625 4650 3625 4750
$Comp
L power:GND #PWR01
U 1 1 5FC7C26E
P 3625 4750
F 0 "#PWR01" H 3625 4500 50  0001 C CNN
F 1 "GND" H 3630 4577 50  0000 C CNN
F 2 "" H 3625 4750 50  0001 C CNN
F 3 "" H 3625 4750 50  0001 C CNN
	1    3625 4750
	1    0    0    -1  
$EndComp
$Comp
L dk_Barrel-Audio-Connectors:SJ-3523-SMT-TR CON1
U 1 1 5FC7E02A
P 5425 5100
F 0 "CON1" H 5483 5487 60  0000 C CNN
F 1 "SJ-3523-SMT-TR" H 5483 5381 60  0000 C CNN
F 2 "digikey-footprints:Switch_Slide_11.6x4mm_SJ-3523-SMT" H 5625 5300 60  0001 L CNN
F 3 "https://www.cui.com/product/resource/digikeypdf/sj-352x-smt_series.pdf" H 5625 5400 60  0001 L CNN
F 4 "CP-3523SJCT-ND" H 5625 5500 60  0001 L CNN "Digi-Key_PN"
F 5 "SJ-3523-SMT-TR" H 5625 5600 60  0001 L CNN "MPN"
F 6 "Connectors, Interconnects" H 5625 5700 60  0001 L CNN "Category"
F 7 "Barrel - Audio Connectors" H 5625 5800 60  0001 L CNN "Family"
F 8 "https://www.cui.com/product/resource/digikeypdf/sj-352x-smt_series.pdf" H 5625 5900 60  0001 L CNN "DK_Datasheet_Link"
F 9 "/product-detail/en/cui-inc/SJ-3523-SMT-TR/CP-3523SJCT-ND/669704" H 5625 6000 60  0001 L CNN "DK_Detail_Page"
F 10 "CONN JACK STEREO 3.5MM SMD R/A" H 5625 6100 60  0001 L CNN "Description"
F 11 "CUI Inc." H 5625 6200 60  0001 L CNN "Manufacturer"
F 12 "Active" H 5625 6300 60  0001 L CNN "Status"
	1    5425 5100
	1    0    0    -1  
$EndComp
Wire Wire Line
	5825 5200 5900 5200
Wire Wire Line
	5900 5200 5900 5300
$Comp
L power:GND #PWR02
U 1 1 5FC802BB
P 5900 5300
F 0 "#PWR02" H 5900 5050 50  0001 C CNN
F 1 "GND" H 5905 5127 50  0000 C CNN
F 2 "" H 5900 5300 50  0001 C CNN
F 3 "" H 5900 5300 50  0001 C CNN
	1    5900 5300
	1    0    0    -1  
$EndComp
Wire Wire Line
	4275 4025 4575 4025
Wire Wire Line
	4275 4125 4575 4125
Wire Wire Line
	5825 5000 6175 5000
Wire Wire Line
	5825 5100 6175 5100
Text Label 4575 4025 0    50   ~ 0
DEBUG_RX
Text Label 4575 4125 0    50   ~ 0
DEBUG_TX
Text Label 6175 5100 0    50   ~ 0
DEBUG_RX
Text Label 6175 5000 0    50   ~ 0
DEBUG_TX
$Comp
L Connector:Conn_ARM_JTAG_SWD_10 J3
U 1 1 5FC879D4
P 5925 3175
F 0 "J3" H 5475 2775 50  0000 R CNN
F 1 "Conn_ARM_JTAG_SWD_10_2.54mm" H 5325 2775 50  0000 R CNN
F 2 "Connector_IDC:IDC-Header_2x05_P2.54mm_Vertical" H 5925 3175 50  0001 C CNN
F 3 "http://infocenter.arm.com/help/topic/com.arm.doc.ddi0314h/DDI0314H_coresight_components_trm.pdf" V 5575 1925 50  0001 C CNN
	1    5925 3175
	-1   0    0    -1  
$EndComp
Connection ~ 5925 2575
Connection ~ 5425 2875
Connection ~ 5425 3175
Connection ~ 5925 3775
Connection ~ 5425 3075
Connection ~ 5425 3275
Connection ~ 6025 3775
$Comp
L Connector:Conn_ARM_JTAG_SWD_10 J2
U 1 1 5FC76906
P 5925 3175
F 0 "J2" H 5475 3575 50  0000 R CNN
F 1 "Conn_ARM_JTAG_SWD_10_1.27mm_Female" H 5325 3325 50  0000 R CNN
F 2 "plib:20021521-00010T1LF" H 5925 3175 50  0001 C CNN
F 3 "http://infocenter.arm.com/help/topic/com.arm.doc.ddi0314h/DDI0314H_coresight_components_trm.pdf" V 5575 1925 50  0001 C CNN
	1    5925 3175
	-1   0    0    -1  
$EndComp
$Comp
L Connector:Conn_ARM_JTAG_SWD_10 J4
U 1 1 5FCA45F2
P 5925 3175
F 0 "J4" H 5450 3325 50  0000 R CNN
F 1 "Conn_ARM_JTAG_SWD_10_1.27mm_Male" H 5325 3575 50  0000 R CNN
F 2 "plib:20021521-00010T1LF" H 5925 3175 50  0001 C CNN
F 3 "http://infocenter.arm.com/help/topic/com.arm.doc.ddi0314h/DDI0314H_coresight_components_trm.pdf" V 5575 1925 50  0001 C CNN
	1    5925 3175
	-1   0    0    -1  
$EndComp
NoConn ~ 5425 3375
$EndSCHEMATC
